.. _lib_bh1749:

BH1749 driver
#############

.. contents::
   :local:
   :depth: 2

You can use the BH1749 driver to measure the illuminance and color temperature of ambient light.
BH1749 is a color sensor IC that senses Red, Green, Blue (RBG) and Infrared and converts them to digital values.
See `BH1749NUC-E`_ for more information about BH1749.

The :ref:`bh1749` sample demonstrates how to run this library in an application.

API documentation
*****************

| Header file: :file:`drivers/sensor/bh1749/bh1749.h`
| Source file: :file:`drivers/sensor/bh1749/bh1749.c`
