.. _cts_client_readme:

GATT Current Time Service (CTS) Client
######################################

.. contents::
   :local:
   :depth: 2

You can use the CTS Client library to retrieve the current time from a connected peer that is running the GATT server with the `Current Time Service <Current Time Service Specification_>`_.

The CTS Client is used in the :ref:`peripheral_cts_client` sample.

API documentation
*****************

| Header file: :file:`include/bluetooth/services/cts_client.h`
| Source file: :file:`subsys/bluetooth/services/cts_client.c`

.. doxygengroup:: bt_gatt_cts_c
   :project: nrf
   :members:
