Package org.libjpegturbo.turbojpeg

## Class TJ

- java.lang.Object
- - org.libjpegturbo.turbojpeg.TJ

-     public final class TJ
      extends java.lang.Object

  TurboJPEG utility class (cannot be instantiated)

- - ### Field Summary

    Fields
    Modifier and Type | Field | Description
    --- | --- | ---
    `static int` | `CS_CMYK` | CMYK colorspace.
    `static int` | `CS_GRAY` | Grayscale colorspace.
    `static int` | `CS_RGB` | RGB colorspace.
    `static int` | `CS_YCbCr` | YCbCr colorspace.
    `static int` | `CS_YCCK` | YCCK colorspace.
    `static int` | `ERR_FATAL` | The error was fatal and non-recoverable.
    `static int` | `ERR_WARNING` | The error was non-fatal and recoverable, but the destination image may still be corrupt.
    `static int` | `FLAG_ACCURATEDCT` | Deprecated. Use `PARAM_FASTDCT` instead.
    `static int` | `FLAG_BOTTOMUP` | Deprecated. Use `PARAM_BOTTOMUP` instead.
    `static int` | `FLAG_FASTDCT` | Deprecated. Use `PARAM_FASTDCT` instead.
    `static int` | `FLAG_FASTUPSAMPLE` | Deprecated. Use `PARAM_FASTUPSAMPLE` instead.
    `static int` | `FLAG_LIMITSCANS` | Deprecated. Use `PARAM_SCANLIMIT` instead.
    `static int` | `FLAG_PROGRESSIVE` | Deprecated. Use `PARAM_PROGRESSIVE` instead.
    `static int` | `FLAG_STOPONWARNING` | Deprecated. Use `PARAM_STOPONWARNING` instead.
    `static int` | `NUMCS` | The number of JPEG colorspaces
    `static int` | `NUMERR` | The number of error codes
    `static int` | `NUMPF` | The number of pixel formats
    `static int` | `NUMSAMP` | The number of chrominance subsampling options
    `static int` | `PARAM_ARITHMETIC` | Arithmetic entropy coding
    `static int` | `PARAM_BOTTOMUP` | Row order in packed-pixel source/destination images
    `static int` | `PARAM_COLORSPACE` | JPEG colorspace
    `static int` | `PARAM_DENSITYUNITS` | JPEG pixel density units
    `static int` | `PARAM_FASTDCT` | DCT/IDCT algorithm [lossy compression and decompression]
    `static int` | `PARAM_FASTUPSAMPLE` | Chrominance upsampling algorithm [lossy decompression only]
    `static int` | `PARAM_JPEGHEIGHT` | JPEG height (in pixels) [decompression only, read-only]
    `static int` | `PARAM_JPEGWIDTH` | JPEG width (in pixels) [decompression only, read-only]
    `static int` | `PARAM_LOSSLESS` | Lossless JPEG
    `static int` | `PARAM_LOSSLESSPSV` | Lossless JPEG predictor selection value (PSV)
    `static int` | `PARAM_LOSSLESSPT` | Lossless JPEG point transform (Pt)
    `static int` | `PARAM_OPTIMIZE` | Optimized baseline entropy coding [lossy compression only]
    `static int` | `PARAM_PRECISION` | JPEG data precision (bits per sample) [decompression only, read-only]
    `static int` | `PARAM_PROGRESSIVE` | Progressive entropy coding
    `static int` | `PARAM_QUALITY` | Perceptual quality of lossy JPEG images [compression only]
    `static int` | `PARAM_RESTARTBLOCKS` | JPEG restart marker interval in MCU blocks (lossy) or samples (lossless) [compression only]
    `static int` | `PARAM_RESTARTROWS` | JPEG restart marker interval in MCU rows (lossy) or sample rows (lossless) [compression only]
    `static int` | `PARAM_SCANLIMIT` | Progressive JPEG scan limit for lossy JPEG images [decompression, lossless transformation]
    `static int` | `PARAM_STOPONWARNING` | Error handling behavior
    `static int` | `PARAM_SUBSAMP` | Chrominance subsampling level
    `static int` | `PARAM_XDENSITY` | JPEG horizontal pixel density
    `static int` | `PARAM_YDENSITY` | JPEG vertical pixel density
    `static int` | `PF_ABGR` | ABGR pixel format.
    `static int` | `PF_ARGB` | ARGB pixel format.
    `static int` | `PF_BGR` | BGR pixel format.
    `static int` | `PF_BGRA` | BGRA pixel format.
    `static int` | `PF_BGRX` | BGRX pixel format.
    `static int` | `PF_CMYK` | CMYK pixel format.
    `static int` | `PF_GRAY` | Grayscale pixel format.
    `static int` | `PF_RGB` | RGB pixel format.
    `static int` | `PF_RGBA` | RGBA pixel format.
    `static int` | `PF_RGBX` | RGBX pixel format.
    `static int` | `PF_XBGR` | XBGR pixel format.
    `static int` | `PF_XRGB` | XRGB pixel format.
    `static int` | `SAMP_411` | 4:1:1 chrominance subsampling.
    `static int` | `SAMP_420` | 4:2:0 chrominance subsampling.
    `static int` | `SAMP_422` | 4:2:2 chrominance subsampling.
    `static int` | `SAMP_440` | 4:4:0 chrominance subsampling.
    `static int` | `SAMP_441` | 4:4:1 chrominance subsampling.
    `static int` | `SAMP_444` | 4:4:4 chrominance subsampling (no chrominance subsampling).
    `static int` | `SAMP_GRAY` | Grayscale.
    `static int` | `SAMP_UNKNOWN` | Unknown subsampling.
    `static java.awt.Rectangle` | `UNCROPPED` | A `java.awt.Rectangle` instance that specifies no cropping
    `static TJScalingFactor` | `UNSCALED` | A `TJScalingFactor` instance that specifies a scaling factor of 1/1 (no scaling)

  - ### Method Summary

    All Methods Static Methods Concrete Methods
    Modifier and Type | Method | Description
    --- | --- | ---
    `static int` | `bufSize​(int width, int height, int jpegSubsamp)` | Returns the maximum size of the buffer (in bytes) required to hold a JPEG image with the given width, height, and level of chrominance subsampling.
    `static int` | `bufSizeYUV​(int width, int align, int height, int subsamp)` | Returns the size of the buffer (in bytes) required to hold a unified planar YUV image with the given width, height, and level of chrominance subsampling.
    `static int` | `getAlphaOffset​(int pixelFormat)` | For the given pixel format, returns the number of samples that the alpha component is offset from the start of the pixel.
    `static int` | `getBlueOffset​(int pixelFormat)` | For the given pixel format, returns the number of samples that the blue component is offset from the start of the pixel.
    `static int` | `getGreenOffset​(int pixelFormat)` | For the given pixel format, returns the number of samples that the green component is offset from the start of the pixel.
    `static int` | `getMCUHeight​(int subsamp)` | Returns the MCU block height for the given level of chrominance subsampling.
    `static int` | `getMCUWidth​(int subsamp)` | Returns the MCU block width for the given level of chrominance subsampling.
    `static int` | `getPixelSize​(int pixelFormat)` | Returns the pixel size (in samples) for the given pixel format.
    `static int` | `getRedOffset​(int pixelFormat)` | For the given pixel format, returns the number of samples that the red component is offset from the start of the pixel.
    `static TJScalingFactor[]` | `getScalingFactors()` | Returns a list of fractional scaling factors that the JPEG decompressor supports.
    `static int` | `planeHeight​(int componentID, int height, int subsamp)` | Returns the plane height of a YUV image plane with the given parameters.
    `static int` | `planeSizeYUV​(int componentID, int width, int stride, int height, int subsamp)` | Returns the size of the buffer (in bytes) required to hold a YUV image plane with the given parameters.
    `static int` | `planeWidth​(int componentID, int width, int subsamp)` | Returns the plane width of a YUV image plane with the given parameters.

    - ### Methods inherited from class java.lang.Object

      `clone, equals, finalize, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

- - ### Field Detail

    - #### NUMSAMP

          public static final int NUMSAMP

      The number of chrominance subsampling options
      See Also:
        Constant Field Values

    - #### SAMP_444

          public static final int SAMP_444

      4:4:4 chrominance subsampling (no chrominance subsampling). The JPEG or YUV image will contain one chrominance component for every pixel in the source image.
      See Also:
        Constant Field Values

    - #### SAMP_422

          public static final int SAMP_422

      4:2:2 chrominance subsampling. The JPEG or YUV image will contain one chrominance component for every 2x1 block of pixels in the source image.
      See Also:
        Constant Field Values

    - #### SAMP_420

          public static final int SAMP_420

      4:2:0 chrominance subsampling. The JPEG or YUV image will contain one chrominance component for every 2x2 block of pixels in the source image.
      See Also:
        Constant Field Values

    - #### SAMP_GRAY

          public static final int SAMP_GRAY

      Grayscale. The JPEG or YUV image will contain no chrominance components.
      See Also:
        Constant Field Values

    - #### SAMP_440

          public static final int SAMP_440

      4:4:0 chrominance subsampling. The JPEG or YUV image will contain one chrominance component for every 1x2 block of pixels in the source image. Note that 4:4:0 subsampling is not fully accelerated in libjpeg-turbo.
      See Also:
        Constant Field Values

    - #### SAMP_411

          public static final int SAMP_411

      4:1:1 chrominance subsampling. The JPEG or YUV image will contain one chrominance component for every 4x1 block of pixels in the source image. JPEG images compressed with 4:1:1 subsampling will be almost exactly the same size as those compressed with 4:2:0 subsampling, and in the aggregate, both subsampling methods produce approximately the same perceptual quality. However, 4:1:1 is better able to reproduce sharp horizontal features. Note that 4:1:1 subsampling is not fully accelerated in libjpeg-turbo.
      See Also:
        Constant Field Values

    - #### SAMP_441

          public static final int SAMP_441

      4:4:1 chrominance subsampling. The JPEG or YUV image will contain one chrominance component for every 1x4 block of pixels in the source image. JPEG images compressed with 4:4:1 subsampling will be almost exactly the same size as those compressed with 4:2:0 subsampling, and in the aggregate, both subsampling methods produce approximately the same perceptual quality. However, 4:4:1 is better able to reproduce sharp vertical features. Note that 4:4:1 subsampling is not fully accelerated in libjpeg-turbo.
      See Also:
        Constant Field Values

    - #### SAMP_UNKNOWN

          public static final int SAMP_UNKNOWN

      Unknown subsampling. The JPEG image uses an unusual type of chrominance subsampling. Such images can be decompressed into packed-pixel images, but they cannot be
      - decompressed into planar YUV images,
      - losslessly transformed if `TJTransform.OPT_CROP` is specified, or
      - partially decompressed using a cropping region.
      See Also:
        Constant Field Values

    - #### NUMPF

          public static final int NUMPF

      The number of pixel formats
      See Also:
        Constant Field Values

    - #### PF_RGB

          public static final int PF_RGB

      RGB pixel format. The red, green, and blue components in the image are stored in 3-sample pixels in the order R, G, B from lowest to highest memory address within each pixel.
      See Also:
        Constant Field Values

    - #### PF_BGR

          public static final int PF_BGR

      BGR pixel format. The red, green, and blue components in the image are stored in 3-sample pixels in the order B, G, R from lowest to highest memory address within each pixel.
      See Also:
        Constant Field Values

    - #### PF_RGBX

          public static final int PF_RGBX

      RGBX pixel format. The red, green, and blue components in the image are stored in 4-sample pixels in the order R, G, B from lowest to highest memory address within each pixel. The X component is ignored when compressing and undefined when decompressing.
      See Also:
        Constant Field Values

    - #### PF_BGRX

          public static final int PF_BGRX

      BGRX pixel format. The red, green, and blue components in the image are stored in 4-sample pixels in the order B, G, R from lowest to highest memory address within each pixel. The X component is ignored when compressing and undefined when decompressing.
      See Also:
        Constant Field Values

    - #### PF_XBGR

          public static final int PF_XBGR

      XBGR pixel format. The red, green, and blue components in the image are stored in 4-sample pixels in the order R, G, B from highest to lowest memory address within each pixel. The X component is ignored when compressing and undefined when decompressing.
      See Also:
        Constant Field Values

    - #### PF_XRGB

          public static final int PF_XRGB

      XRGB pixel format. The red, green, and blue components in the image are stored in 4-sample pixels in the order B, G, R from highest to lowest memory address within each pixel. The X component is ignored when compressing and undefined when decompressing.
      See Also:
        Constant Field Values

    - #### PF_GRAY

          public static final int PF_GRAY

      Grayscale pixel format. Each 1-sample pixel represents a luminance (brightness) level from 0 to the maximum sample value (255 for 8-bit samples, 4095 for 12-bit samples, and 65535 for 16-bit samples.)
      See Also:
        Constant Field Values

    - #### PF_RGBA

          public static final int PF_RGBA

      RGBA pixel format. This is the same as `PF_RGBX`, except that when decompressing, the X component is guaranteed to be equal to the maximum sample value, which can be interpreted as an opaque alpha channel.
      See Also:
        Constant Field Values

    - #### PF_BGRA

          public static final int PF_BGRA

      BGRA pixel format. This is the same as `PF_BGRX`, except that when decompressing, the X component is guaranteed to be equal to the maximum sample value, which can be interpreted as an opaque alpha channel.
      See Also:
        Constant Field Values

    - #### PF_ABGR

          public static final int PF_ABGR

      ABGR pixel format. This is the same as `PF_XBGR`, except that when decompressing, the X component is guaranteed to be equal to the maximum sample value, which can be interpreted as an opaque alpha channel.
      See Also:
        Constant Field Values

    - #### PF_ARGB

          public static final int PF_ARGB

      ARGB pixel format. This is the same as `PF_XRGB`, except that when decompressing, the X component is guaranteed to be equal to the maximum sample value, which can be interpreted as an opaque alpha channel.
      See Also:
        Constant Field Values

    - #### PF_CMYK

          public static final int PF_CMYK

      CMYK pixel format. Unlike RGB, which is an additive color model used primarily for display, CMYK (Cyan/Magenta/Yellow/Key) is a subtractive color model used primarily for printing. In the CMYK color model, the value of each color component typically corresponds to an amount of cyan, magenta, yellow, or black ink that is applied to a white background. In order to convert between CMYK and RGB, it is necessary to use a color management system (CMS.) A CMS will attempt to map colors within the printer's gamut to perceptually similar colors in the display's gamut and vice versa, but the mapping is typically not 1:1 or reversible, nor can it be defined with a simple formula. Thus, such a conversion is out of scope for a codec library. However, the TurboJPEG API allows for compressing packed-pixel CMYK images into YCCK JPEG images (see `CS_YCCK`) and decompressing YCCK JPEG images into packed-pixel CMYK images.
      See Also:
        Constant Field Values

    - #### NUMCS

          public static final int NUMCS

      The number of JPEG colorspaces
      See Also:
        Constant Field Values

    - #### CS_RGB

          public static final int CS_RGB

      RGB colorspace. When compressing the JPEG image, the R, G, and B components in the source image are reordered into image planes, but no colorspace conversion or subsampling is performed. RGB JPEG images can be compressed from and decompressed to packed-pixel images with any of the extended RGB or grayscale pixel formats, but they cannot be compressed from or decompressed to planar YUV images.
      See Also:
        Constant Field Values

    - #### CS_YCbCr

          public static final int CS_YCbCr

      YCbCr colorspace. YCbCr is not an absolute colorspace but rather a mathematical transformation of RGB designed solely for storage and transmission. YCbCr images must be converted to RGB before they can actually be displayed. In the YCbCr colorspace, the Y (luminance) component represents the black & white portion of the original image, and the Cb and Cr (chrominance) components represent the color portion of the original image. Originally, the analog equivalent of this transformation allowed the same signal to drive both black & white and color televisions, but JPEG images use YCbCr primarily because it allows the color data to be optionally subsampled for the purposes of reducing network or disk usage. YCbCr is the most common JPEG colorspace, and YCbCr JPEG images can be compressed from and decompressed to packed-pixel images with any of the extended RGB or grayscale pixel formats. YCbCr JPEG images can also be compressed from and decompressed to planar YUV images.
      See Also:
        Constant Field Values

    - #### CS_GRAY

          public static final int CS_GRAY

      Grayscale colorspace. The JPEG image retains only the luminance data (Y component), and any color data from the source image is discarded. Grayscale JPEG images can be compressed from and decompressed to packed-pixel images with any of the extended RGB or grayscale pixel formats, or they can be compressed from and decompressed to planar YUV images.
      See Also:
        Constant Field Values

    - #### CS_CMYK

          public static final int CS_CMYK

      CMYK colorspace. When compressing the JPEG image, the C, M, Y, and K components in the source image are reordered into image planes, but no colorspace conversion or subsampling is performed. CMYK JPEG images can only be compressed from and decompressed to packed-pixel images with the CMYK pixel format.
      See Also:
        Constant Field Values

    - #### CS_YCCK

          public static final int CS_YCCK

      YCCK colorspace. YCCK (AKA "YCbCrK") is not an absolute colorspace but rather a mathematical transformation of CMYK designed solely for storage and transmission. It is to CMYK as YCbCr is to RGB. CMYK pixels can be reversibly transformed into YCCK, and as with YCbCr, the chrominance components in the YCCK pixels can be subsampled without incurring major perceptual loss. YCCK JPEG images can only be compressed from and decompressed to packed-pixel images with the CMYK pixel format.
      See Also:
        Constant Field Values

    - #### PARAM_STOPONWARNING

          public static final int PARAM_STOPONWARNING

      Error handling behavior

      Value

      - `0` [default] Allow the current compression/decompression/transform operation to complete unless a fatal error is encountered.
      - `1` Immediately discontinue the current compression/decompression/transform operation if a warning (non-fatal error) occurs.
      See Also:
        Constant Field Values

    - #### PARAM_BOTTOMUP

          public static final int PARAM_BOTTOMUP

      Row order in packed-pixel source/destination images

      Value

      - `0` [default] top-down (X11) order
      - `1` bottom-up (Windows, OpenGL) order
      See Also:
        Constant Field Values

    - #### PARAM_QUALITY

          public static final int PARAM_QUALITY

      Perceptual quality of lossy JPEG images [compression only]

      Value

      - `1`-`100` (`1` = worst quality but best compression, `100` = best quality but worst compression) [no default; must be explicitly specified]
      See Also:
        Constant Field Values

    - #### PARAM_SUBSAMP

          public static final int PARAM_SUBSAMP

      Chrominance subsampling level

      The JPEG or YUV image uses (decompression, decoding) or will use (lossy compression, encoding) the specified level of chrominance subsampling.

      When pixels are converted from RGB to YCbCr (see `CS_YCbCr`) or from CMYK to YCCK (see `CS_YCCK`) as part of the JPEG compression process, some of the Cb and Cr (chrominance) components can be discarded or averaged together to produce a smaller image with little perceptible loss of image clarity. (The human eye is more sensitive to small changes in brightness than to small changes in color.) This is called "chrominance subsampling".

      Value

      - One of `TJ.SAMP_*` [no default; must be explicitly specified for lossy compression, encoding, and decoding]
      See Also:
        Constant Field Values

    - #### PARAM_JPEGWIDTH

          public static final int PARAM_JPEGWIDTH

      JPEG width (in pixels) [decompression only, read-only]
      See Also:
        Constant Field Values

    - #### PARAM_JPEGHEIGHT

          public static final int PARAM_JPEGHEIGHT

      JPEG height (in pixels) [decompression only, read-only]
      See Also:
        Constant Field Values

    - #### PARAM_PRECISION

          public static final int PARAM_PRECISION

      JPEG data precision (bits per sample) [decompression only, read-only]

      The JPEG image uses the specified number of bits per sample.

      Value

      - `8`, `12`, or `16`

      12-bit data precision implies `PARAM_OPTIMIZE` unless `PARAM_ARITHMETIC` is set.

      See Also:
        Constant Field Values

    - #### PARAM_COLORSPACE

          public static final int PARAM_COLORSPACE

      JPEG colorspace

      The JPEG image uses (decompression) or will use (lossy compression) the specified colorspace.

      Value

      - One of `TJ.CS_*` [default for lossy compression: automatically selected based on the subsampling level and pixel format]
      See Also:
        Constant Field Values

    - #### PARAM_FASTUPSAMPLE

          public static final int PARAM_FASTUPSAMPLE

      Chrominance upsampling algorithm [lossy decompression only]

      Value

      - `0` [default] Use smooth upsampling when decompressing a JPEG image that was compressed using chrominance subsampling. This creates a smooth transition between neighboring chrominance components in order to reduce upsampling artifacts in the decompressed image.
      - `1` Use the fastest chrominance upsampling algorithm available, which may combine upsampling with color conversion.
      See Also:
        Constant Field Values

    - #### PARAM_FASTDCT

          public static final int PARAM_FASTDCT

      DCT/IDCT algorithm [lossy compression and decompression]

      Value

      - `0` [default] Use the most accurate DCT/IDCT algorithm available.
      - `1` Use the fastest DCT/IDCT algorithm available.

      This parameter is provided mainly for backward compatibility with libjpeg, which historically implemented several different DCT/IDCT algorithms because of performance limitations with 1990s CPUs. In the libjpeg-turbo implementation of the TurboJPEG API:

      - The "fast" and "accurate" DCT/IDCT algorithms perform similarly on modern x86/x86-64 CPUs that support AVX2 instructions.
      - The "fast" algorithm is generally only about 5-15% faster than the "accurate" algorithm on other types of CPUs.
      - The difference in accuracy between the "fast" and "accurate" algorithms is the most pronounced at JPEG quality levels above 90 and tends to be more pronounced with decompression than with compression.
      - The "fast" algorithm degrades and is not fully accelerated for JPEG quality levels above 97, so it will be slower than the "accurate" algorithm.
      See Also:
        Constant Field Values

    - #### PARAM_OPTIMIZE

          public static final int PARAM_OPTIMIZE

      Optimized baseline entropy coding [lossy compression only]

      Value

      - `0` [default] The JPEG image will use the default Huffman tables.
      - `1` Optimal Huffman tables will be computed for the JPEG image. For lossless transformation, this can also be specified using `TJTransform.OPT_OPTIMIZE`.

      Optimized baseline entropy coding will improve compression slightly (generally 5% or less), but it will reduce compression performance considerably.

      See Also:
        Constant Field Values

    - #### PARAM_PROGRESSIVE

          public static final int PARAM_PROGRESSIVE

      Progressive entropy coding

      Value

      - `0` [default for compression, lossless transformation] The lossy JPEG image uses (decompression) or will use (compression, lossless transformation) baseline entropy coding.
      - `1` The lossy JPEG image uses (decompression) or will use (compression, lossless transformation) progressive entropy coding. For lossless transformation, this can also be specified using `TJTransform.OPT_PROGRESSIVE`.

      Progressive entropy coding will generally improve compression relative to baseline entropy coding, but it will reduce compression and decompression performance considerably. Can be combined with `PARAM_ARITHMETIC`. Implies `PARAM_OPTIMIZE` unless `PARAM_ARITHMETIC` is also set.

      See Also:
        Constant Field Values

    - #### PARAM_SCANLIMIT

          public static final int PARAM_SCANLIMIT

      Progressive JPEG scan limit for lossy JPEG images [decompression, lossless transformation]

      Setting this parameter will cause the decompression and transform functions to return an error if the number of scans in a progressive JPEG image exceeds the specified limit. The primary purpose of this is to allow security-critical applications to guard against an exploit of the progressive JPEG format described in this report.

      Value

      - maximum number of progressive JPEG scans that the decompression and transform functions will process [default: `0` (no limit)]
      See Also:
        `PARAM_PROGRESSIVE`, Constant Field Values

    - #### PARAM_ARITHMETIC

          public static final int PARAM_ARITHMETIC

      Arithmetic entropy coding

      Value

      - `0` [default for compression, lossless transformation] The lossy JPEG image uses (decompression) or will use (compression, lossless transformation) Huffman entropy coding.
      - `1` The lossy JPEG image uses (decompression) or will use (compression, lossless transformation) arithmetic entropy coding. For lossless transformation, this can also be specified using `TJTransform.OPT_ARITHMETIC`.

      Arithmetic entropy coding will generally improve compression relative to Huffman entropy coding, but it will reduce compression and decompression performance considerably. Can be combined with `PARAM_PROGRESSIVE`.

      See Also:
        Constant Field Values

    - #### PARAM_LOSSLESS

          public static final int PARAM_LOSSLESS

      Lossless JPEG

      Value

      - `0` [default for compression] The JPEG image is (decompression) or will be (compression) lossy/DCT-based.
      - `1` The JPEG image is (decompression) or will be (compression) lossless/predictive.

      In most cases, compressing and decompressing lossless JPEG images is considerably slower than compressing and decompressing lossy JPEG images. Also note that the following features are not available with lossless JPEG images:

      - Colorspace conversion (lossless JPEG images always use `CS_RGB`, `CS_GRAY`, or `CS_CMYK`, depending on the pixel format of the source image)
      - Chrominance subsampling (lossless JPEG images always use `SAMP_444`)
      - JPEG quality selection
      - DCT/IDCT algorithm selection
      - Progressive entropy coding
      - Arithmetic entropy coding
      - Compression from/decompression to planar YUV images
      - Decompression scaling
      - Lossless transformation
      See Also:
        `PARAM_LOSSLESSPSV`, `PARAM_LOSSLESSPT`, Constant Field Values

    - #### PARAM_LOSSLESSPSV

          public static final int PARAM_LOSSLESSPSV

      Lossless JPEG predictor selection value (PSV)

      Value

      - `1`-`7` [default for compression: `1`]
      See Also:
        `PARAM_LOSSLESS`, Constant Field Values

    - #### PARAM_LOSSLESSPT

          public static final int PARAM_LOSSLESSPT

      Lossless JPEG point transform (Pt)

      Value

      - `0` through precision - 1, where precision is the JPEG data precision in bits [default for compression: `0`]

      A point transform value of `0` is necessary in order to generate a fully lossless JPEG image. (A non-zero point transform value right-shifts the input samples by the specified number of bits, which is effectively a form of lossy color quantization.)

      See Also:
        `PARAM_LOSSLESS`, `PARAM_PRECISION`, Constant Field Values

    - #### PARAM_RESTARTBLOCKS

          public static final int PARAM_RESTARTBLOCKS

      JPEG restart marker interval in MCU blocks (lossy) or samples (lossless) [compression only]

      The nature of entropy coding is such that a corrupt JPEG image cannot be decompressed beyond the point of corruption unless it contains restart markers. A restart marker stops and restarts the entropy coding algorithm so that, if a JPEG image is corrupted, decompression can resume at the next marker. Thus, adding more restart markers improves the fault tolerance of the JPEG image, but adding too many restart markers can adversely affect the compression ratio and performance.

      Value

      - the number of MCU blocks or samples between each restart marker [default: `0` (no restart markers)]

      Setting this parameter to a non-zero value sets `PARAM_RESTARTROWS` to 0.

      See Also:
        Constant Field Values

    - #### PARAM_RESTARTROWS

          public static final int PARAM_RESTARTROWS

      JPEG restart marker interval in MCU rows (lossy) or sample rows (lossless) [compression only]

      See `PARAM_RESTARTBLOCKS` for a description of restart markers.

      Value

      - the number of MCU rows or sample rows between each restart marker [default: `0` (no restart markers)]

      Setting this parameter to a non-zero value sets `PARAM_RESTARTBLOCKS` to 0.

      See Also:
        Constant Field Values

    - #### PARAM_XDENSITY

          public static final int PARAM_XDENSITY

      JPEG horizontal pixel density

      Value

      - The JPEG image has (decompression) or will have (compression) the specified horizontal pixel density [default for compression: `1`].

      This value is stored in or read from the JPEG header. It does not affect the contents of the JPEG image.

      See Also:
        `PARAM_DENSITYUNITS`, Constant Field Values

    - #### PARAM_YDENSITY

          public static final int PARAM_YDENSITY

      JPEG vertical pixel density

      Value

      - The JPEG image has (decompression) or will have (compression) the specified vertical pixel density [default for compression: `1`].

      This value is stored in or read from the JPEG header. It does not affect the contents of the JPEG image.

      See Also:
        `PARAM_DENSITYUNITS`, Constant Field Values

    - #### PARAM_DENSITYUNITS

          public static final int PARAM_DENSITYUNITS

      JPEG pixel density units

      Value

      - `0` [default for compression] The pixel density of the JPEG image is expressed (decompression) or will be expressed (compression) in unknown units.
      - `1` The pixel density of the JPEG image is expressed (decompression) or will be expressed (compression) in units of pixels/inch.
      - `2` The pixel density of the JPEG image is expressed (decompression) or will be expressed (compression) in units of pixels/cm.

      This value is stored in or read from the JPEG header. It does not affect the contents of the JPEG image.

      See Also:
        `PARAM_XDENSITY`, `PARAM_YDENSITY`, Constant Field Values

    - #### FLAG_BOTTOMUP

          @Deprecated
          public static final int FLAG_BOTTOMUP

      Deprecated.
      Use `PARAM_BOTTOMUP` instead.
      See Also:
        Constant Field Values

    - #### FLAG_FASTUPSAMPLE

          @Deprecated
          public static final int FLAG_FASTUPSAMPLE

      Deprecated.
      Use `PARAM_FASTUPSAMPLE` instead.
      See Also:
        Constant Field Values

    - #### FLAG_FASTDCT

          @Deprecated
          public static final int FLAG_FASTDCT

      Deprecated.
      Use `PARAM_FASTDCT` instead.
      See Also:
        Constant Field Values

    - #### FLAG_ACCURATEDCT

          @Deprecated
          public static final int FLAG_ACCURATEDCT

      Deprecated.
      Use `PARAM_FASTDCT` instead.
      See Also:
        Constant Field Values

    - #### FLAG_STOPONWARNING

          @Deprecated
          public static final int FLAG_STOPONWARNING

      Deprecated.
      Use `PARAM_STOPONWARNING` instead.
      See Also:
        Constant Field Values

    - #### FLAG_PROGRESSIVE

          @Deprecated
          public static final int FLAG_PROGRESSIVE

      Deprecated.
      Use `PARAM_PROGRESSIVE` instead.
      See Also:
        Constant Field Values

    - #### FLAG_LIMITSCANS

          @Deprecated
          public static final int FLAG_LIMITSCANS

      Deprecated.
      Use `PARAM_SCANLIMIT` instead.
      See Also:
        Constant Field Values

    - #### NUMERR

          public static final int NUMERR

      The number of error codes
      See Also:
        Constant Field Values

    - #### ERR_WARNING

          public static final int ERR_WARNING

      The error was non-fatal and recoverable, but the destination image may still be corrupt.

      NOTE: due to the design of the TurboJPEG Java API, only certain methods (specifically, `TJDecompressor.decompress*()` methods with a void return type) will complete and leave the destination image in a fully recoverable state after a non-fatal error occurs.

      See Also:
        Constant Field Values

    - #### ERR_FATAL

          public static final int ERR_FATAL

      The error was fatal and non-recoverable.
      See Also:
        Constant Field Values

    - #### UNSCALED

          public static final TJScalingFactor UNSCALED

      A `TJScalingFactor` instance that specifies a scaling factor of 1/1 (no scaling)

    - #### UNCROPPED

          public static final java.awt.Rectangle UNCROPPED

      A `java.awt.Rectangle` instance that specifies no cropping

  - ### Method Detail

    - #### getMCUWidth

          public static int getMCUWidth​(int subsamp)

      Returns the MCU block width for the given level of chrominance subsampling.
      Parameters:
        `subsamp` - the level of chrominance subsampling (one of `SAMP_*`)
      Returns:
        the MCU block width for the given level of chrominance subsampling.

    - #### getMCUHeight

          public static int getMCUHeight​(int subsamp)

      Returns the MCU block height for the given level of chrominance subsampling.
      Parameters:
        `subsamp` - the level of chrominance subsampling (one of `SAMP_*`)
      Returns:
        the MCU block height for the given level of chrominance subsampling.

    - #### getPixelSize

          public static int getPixelSize​(int pixelFormat)

      Returns the pixel size (in samples) for the given pixel format.
      Parameters:
        `pixelFormat` - the pixel format (one of `PF_*`)
      Returns:
        the pixel size (in samples) for the given pixel format.

    - #### getRedOffset

          public static int getRedOffset​(int pixelFormat)

      For the given pixel format, returns the number of samples that the red component is offset from the start of the pixel. For instance, if an 8-bit-per-sample pixel of format `TJ.PF_BGRX` is stored in `char pixel[]`, then the red component will be `pixel[TJ.getRedOffset(TJ.PF_BGRX)]`.
      Parameters:
        `pixelFormat` - the pixel format (one of `PF_*`)
      Returns:
        the red offset for the given pixel format, or -1 if the pixel format does not have a red component.

    - #### getGreenOffset

          public static int getGreenOffset​(int pixelFormat)

      For the given pixel format, returns the number of samples that the green component is offset from the start of the pixel. For instance, if an 8-bit-per-sample pixel of format `TJ.PF_BGRX` is stored in `char pixel[]`, then the green component will be `pixel[TJ.getGreenOffset(TJ.PF_BGRX)]`.
      Parameters:
        `pixelFormat` - the pixel format (one of `PF_*`)
      Returns:
        the green offset for the given pixel format, or -1 if the pixel format does not have a green component.

    - #### getBlueOffset

          public static int getBlueOffset​(int pixelFormat)

      For the given pixel format, returns the number of samples that the blue component is offset from the start of the pixel. For instance, if an 8-bit-per-sample pixel of format `TJ.PF_BGRX` is stored in `char pixel[]`, then the blue component will be `pixel[TJ.getBlueOffset(TJ.PF_BGRX)]`.
      Parameters:
        `pixelFormat` - the pixel format (one of `PF_*`)
      Returns:
        the blue offset for the given pixel format, or -1 if the pixel format does not have a blue component.

    - #### getAlphaOffset

          public static int getAlphaOffset​(int pixelFormat)

      For the given pixel format, returns the number of samples that the alpha component is offset from the start of the pixel. For instance, if an 8-bit-per-sample pixel of format `TJ.PF_BGRA` is stored in `char pixel[]`, then the alpha component will be `pixel[TJ.getAlphaOffset(TJ.PF_BGRA)]`.
      Parameters:
        `pixelFormat` - the pixel format (one of `PF_*`)
      Returns:
        the alpha offset for the given pixel format, or -1 if the pixel format does not have a alpha component.

    - #### bufSize

          public static int bufSize​(int width,
                                    int height,
                                    int jpegSubsamp)

      Returns the maximum size of the buffer (in bytes) required to hold a JPEG image with the given width, height, and level of chrominance subsampling.
      Parameters:
        `width` - the width (in pixels) of the JPEG image
        `height` - the height (in pixels) of the JPEG image
        `jpegSubsamp` - the level of chrominance subsampling to be used when generating the JPEG image (one of `TJ.SAMP_*`.) `SAMP_UNKNOWN` is treated like `SAMP_444`, since a buffer large enough to hold a JPEG image with no subsampling should also be large enough to hold a JPEG image with an arbitrary level of subsampling. Note that lossless JPEG images always use `SAMP_444`.
      Returns:
        the maximum size of the buffer (in bytes) required to hold a JPEG image with the given width, height, and level of chrominance subsampling.

    - #### bufSizeYUV

          public static int bufSizeYUV​(int width,
                                       int align,
                                       int height,
                                       int subsamp)

      Returns the size of the buffer (in bytes) required to hold a unified planar YUV image with the given width, height, and level of chrominance subsampling.
      Parameters:
        `width` - the width (in pixels) of the YUV image
        `align` - row alignment (in bytes) of the YUV image (must be a power of 2.) Setting this parameter to n specifies that each row in each plane of the YUV image will be padded to the nearest multiple of n bytes (1 = unpadded.)
        `height` - the height (in pixels) of the YUV image
        `subsamp` - the level of chrominance subsampling used in the YUV image (one of `TJ.SAMP_*`)
      Returns:
        the size of the buffer (in bytes) required to hold a unified planar YUV image with the given width, height, and level of chrominance subsampling.

    - #### planeSizeYUV

          public static int planeSizeYUV​(int componentID,
                                         int width,
                                         int stride,
                                         int height,
                                         int subsamp)

      Returns the size of the buffer (in bytes) required to hold a YUV image plane with the given parameters.
      Parameters:
        `componentID` - ID number of the image plane (0 = Y, 1 = U/Cb, 2 = V/Cr)
        `width` - width (in pixels) of the YUV image. NOTE: this is the width of the whole image, not the plane width.
        `stride` - bytes per row in the image plane.
        `height` - height (in pixels) of the YUV image. NOTE: this is the height of the whole image, not the plane height.
        `subsamp` - the level of chrominance subsampling used in the YUV image (one of `TJ.SAMP_*`)
      Returns:
        the size of the buffer (in bytes) required to hold a YUV image plane with the given parameters.

    - #### planeWidth

          public static int planeWidth​(int componentID,
                                       int width,
                                       int subsamp)

      Returns the plane width of a YUV image plane with the given parameters. Refer to `YUVImage` for a description of plane width.
      Parameters:
        `componentID` - ID number of the image plane (0 = Y, 1 = U/Cb, 2 = V/Cr)
        `width` - width (in pixels) of the YUV image
        `subsamp` - the level of chrominance subsampling used in the YUV image (one of `TJ.SAMP_*`)
      Returns:
        the plane width of a YUV image plane with the given parameters.

    - #### planeHeight

          public static int planeHeight​(int componentID,
                                        int height,
                                        int subsamp)

      Returns the plane height of a YUV image plane with the given parameters. Refer to `YUVImage` for a description of plane height.
      Parameters:
        `componentID` - ID number of the image plane (0 = Y, 1 = U/Cb, 2 = V/Cr)
        `height` - height (in pixels) of the YUV image
        `subsamp` - the level of chrominance subsampling used in the YUV image (one of `TJ.SAMP_*`)
      Returns:
        the plane height of a YUV image plane with the given parameters.

    - #### getScalingFactors

          public static TJScalingFactor[] getScalingFactors()

      Returns a list of fractional scaling factors that the JPEG decompressor supports.
      Returns:
        a list of fractional scaling factors that the JPEG decompressor supports.