# Debugger: Control and Machine State

This plugin presents actions for controlling targets and modifying machine state. It provides a drop-down action in the main toolbar for choosing what to control for the current target: The live target, the integrated emulator, or the recorded trace. Only those control actions suitable for the selection are displayed. Machine-state edits and breakpoint commands throughout the UI are directed accordingly.

## Actions

The plugin provides several actions, but only certain ones are displayed, depending on the current mode.

### Control Mode

This action changes the mode for the active trace and, if applicable, its associated live target. It is always displayed, but only available when a trace is active. The possible modes are:

- Control Target w/Edits Disabled: The default, this presents actions for controlling the live target but rejects all machine-state edits. Breakpoint commands are directed to the live target. When active, the UI automatically follows the latest snapshot recorded, and navigating back in time is not permitted. If the target is terminated and the trace remains open, the mode is automatically switched to Control Trace.
- Control Target: This presents actions for controlling the live target and directs edits to the live target. Breakpoint commands are directed to the live target. When active, the UI automatically follows the latest snapshot recorded, an navigating back in time is not permitted. If the target is terminated and the trace remains open, the mode is automatically switched to Control Emulator.
- Control Trace w/Edits Disabled: This presents actions for navigating trace snapshots but rejects all machine-state edits. Breakpoint commands are directed to the emulator.
- Control Trace: This presents actions for navigating trace snapshots. It directs all edits to the trace database. Edits are generally always accepted, and they are applied directly to the trace. Breakpoint commands are directed to the emulator.
- Control Emulator: This presents actions for controlling the integrated emulator. Breakpoint commands are directed to the emulator. This can be used for interpolating and extrapolating execution from the current snapshot, without affecting the live target. It directs edits to the integrated emulator by generating patch steps and appending them to the emulation schedule. See the Go To Time action. Essentially, the change is applied in the trace's scratch space, leaving the original recording in tact. Due to implementation details, a thread must be selected, even if edits only affect memory. Additionally, the disassembly context register cannot be modified.

## Target Control Actions

These actions are visible when a Control Target mode is selected. They are available only when the current trace has an associated live target. Commands are directed to the focused object or a suitable substitute.

### Resume

Allow the current target to resume execution. Other debuggers may call this "continue" or "go." If successful, the target enters the "running" state until it is interrupted or terminated. This is available when the target is currently stopped.

### Interrupt

Interrupt the current target's execution. Other debuggers may call this "break," "suspend," or "stop." If successful, the target enters the "stopped" state. This is available when the target is currently running.

### Kill

Kill the current target. Other debuggers may call this "terminate" or "stop." This may consequently close the current trace. If successful, the target enters the "terminated" state. This is always available for a live target.

### Disconnect

Disconnect from the current target's debugger. This usually causes the connected debugger to terminate and likely kill its targets. This may consequently close the current trace (and perhaps others). This is always available for a live target.

### Step Into

Step the current target to the next instruction. This is available when the target is currently stopped. If successful the target may briefly enter the "running" state.

### Step Over

Step the current target to the next instruction in the current subroutine. This is available when the target is currently stopped. If successful the target may briefly enter the "running" state.

### Step Out

Allow the current target to finish the current subroutine, pausing after. This is available when the target is currently stopped. If successful the target may briefly enter the "running" state.

### Step Extended (Repeat Last)

Perform a target-defined step, perhaps the last (possibly custom) step. This is available when the target is currently stopped. If successful the target may briefly enter the "running" state.

## Trace Navigation Actions

These actions are visible when a Control Trace mode is selected. They are available when there is an active trace.

### Snapshot Backward

This activates the previous snapshot. All windows displaying machine state will show that recorded in the activated snapshot. This is available only when there exists a snapshot previous to the current.

### Snapshot Forward

This activates the next snapshot. All windows displaying machine state will show that recorded in the activated snapshot. This is available only when there exists a snapshot after the current.

## Emulation Actions

These actions are visible when the Control Emulator mode is selected. They are available when there is an active trace. Commands are directed to the integrated emulator for the current trace.

### Resume

Allow the emulator to resume execution. This is available when no other integrated emulator is running. A monitor dialog is presented during execution, but the GUI remains responsive. Only one emulator can be run from the GUI at a time. If the current snapshot represents the live target, the emulator may read additional machine state from the live target. For non-contrived programs, the emulator will likely be interrupted, since some instructions and system calls are not yet supported. It could also start executing from unmapped memory or enter an infinite loop. If it seems to carry on too long, interrupt it and examine.

### Interrupt

Interrupt the currently-running emulator. This is available when any integrated emulator is running. In most cases, this is the emulator for the current trace, but it may not be. Canceling the dialog for an emulation task will also interrupt the emulator. Upon interruption, the emulation schedule is noted and the snapshot displayed in the GUI.

### Step Back

Steps the emulator to the previous instruction, by flow. This is available when the current snapshot includes emulated steps. This operates by repeating the current emulation schedule with one less step. Thus, it effectively steps backward, heeding the proper control flow. While not common, if emulation to the current snapshot took a good bit of time, then stepping backward will likely take about the same amount of time.

### Step Into

Steps the emulator to the next instruction, by flow. This is available when there is an active thread. At worst, this operates by repeating the current emulation schedule with one more step of the current thread. In most cases, this can use the cached emulator for the current snapshot and advance it a single step. Note that "Step Over" is not currently supported by the emulator.

### Skip Over

Skips the emulator over the current instruction, ignoring flow. This is available when there is an active thread. At worst, this operates by repeating the current emulation schedule with an added skip for the current thread. In most cases, this can use the cached emulator for the current snapshot and advance it by skipping once. Note that this skips the instruction. Thus, when used on a "call" instruction, all effects and side-effects of the subroutine are averted. This is not the same as "Step Over," which is not currently supported by the emulator.

## Recommendations

The default mode is Control Target w/Edits Disabled, because in most cases, this is the desired behavior. When the target dies, the mode becomes Control Trace w/Edits Disabled. For the most part, modifying the recorded trace itself is discouraged. There are few reasons to edit a trace, perhaps including 1) Hand-generating an experimental trace; 2) Generating a trace from a script, e.g., importing an event log, recording an emulated target; 3) Patching in state missed by the original recording. Be wary of Control Trace mode, especially after emulating, since you could accidentally edit scratch space in the trace. It is allowed but can produce non-intuitive and erroneous results, since the emulator caches its snapshots in scratch space.

To modify state in a live target, use the Control Target mode. NOTE: Some UI components will also require you to toggle a write protector. This also affects scripts that use the state editing service. However, disabling edits cannot prevent a script from directly accessing Ghidra's Target API to modify a target. Nor can it prevent edits via the connected debugger's command-line interpreter. The following components all use the service: Dynamic Listing, Memory (Dynamic Bytes), Registers, and Watches.