Example file
InflowWind driver input file.
   t           echo           -- whether this input file should be echoed to a file (flag)
===============================================================================
"inflowwind_example.dat"  IfWFileName    -- Name of InflowWind input file (-)
===================== File Conversion Options =================================
 false         WrHAWC         -- Convert all data to HAWC2 format? (flag)
 false         WrBladed       -- Convert all data to Bladed format? (flag)
 false         WrVTK          -- Convert all data to VTK format? (flag)
 false         WrUniform      -- Convert data to Uniform wind format? (flag)
=====================  Tests of Interpolation Options =========================
   DEFAULT     NumTSteps      -- number of timesteps to run (DEFAULT for all) (-)
   0.0         TStart         -- Start time (s)
   DEFAULT     DT             -- timestep size for driver to take (s, or DEFAULT for what the file contains)
   t           Summary        -- Summarize the data extents in the windfile (flag)
   t           SummaryFile    -- Write summary to file (.dvr.sum) (flag)
   f           BoxExceedAllow -- Allow point sampling outside grid
----  Points file input (output given as POINTSFILENAME.Velocity.dat) --------
   f           PointsFile     -- read in a list of output points from a file (flag)
"Test005.txt"  PointsFileName -- name of points file (-) (comma separated x,y,z coordinates, # symbol for comments)
   f           CalcAccel      -- calculate and output acceleration at points in addition to velocity
----  Output grid (Points below ground will simply be ignored) ---------------
   t           WindGrid       -- report wind data at set of X,Y,Z coordinat            (flag)
   6,0,15      GridCtrCoord   -- coordinate of center of grid                          (m)
   1,1,0       GridDx,GridDY,GridDZ  -- Step size of grid                              (m)
   1,1,0       GridNx,GridNY,GridNZ  -- number of grid points in X, Y and Z directions (-)
----  Output VTK slices  ------------------------------------------------------
   0            NOutWindXY    -- Number of XY planes for output <RootName>.XY<loc>.t<n>.vtk (-) [0 to 9]
   90           OutWindZ      -- Z coordinates of XY planes for output (m) [1 to NOutWindXY] [unused for NOutWindXY=0]
   0            NOutWindXZ    -- Number of XZ planes for output <RootName>.YZ<loc>.t<n>.vtk (-) [0 to 9]
   0            OutWindY      -- Y coordinates of XZ planes for output (m) [1 to NOutWindXZ] [unused for NOutWindXZ=0]
   0            NOutWindYZ    -- Number of YZ planes for output <RootName>.YZ<loc>.t<n>.vtk (-) [0 to 9]
   0            OutWindX      -- X coordinates of YZ planes for output (m) [1 to NOutWindYZ] [unused for NOutWindYZ=0]
END of driver input file
