------- InflowWind INPUT FILE -------------------------------------------------------------------------
Example of InflowWind input file for OpenFAST
---------------------------------------------------------------------------------------------------------------
False         Echo           - Echo input data to <RootName>.ech (flag)
          3   WindType       - switch for wind file type (1=steady; 2=uniform; 3=binary TurbSim FF; 4=binary Bladed-style FF; 5=HAWC format; 6=User defined; 7=native Bladed FF)
          0   PropagationDir - Direction of wind propagation (meteorological rotation from aligned with X (positive rotates towards -Y) -- degrees) (not used for native Bladed format WindType=7)
          0   VFlowAng       - Upflow angle (degrees) (not used for native Bladed format WindType=7)
      False   VelInterpCubic - Use cubic interpolation for velocity in time (false=linear, true=cubic) [Used with WindType=2,3,4,5,7]
          1   NWindVel       - Number of points to output the wind velocity    (0 to 9)
          0   WindVxiList    - List of coordinates in the inertial X direction (m)
          0   WindVyiList    - List of coordinates in the inertial Y direction (m)
         90   WindVziList    - List of coordinates in the inertial Z direction (m)
================== Parameters for Steady Wind Conditions [used only for WindType = 1] =========================
          0   HWindSpeed     - Horizontal wind speed                           (m/s)
         90   RefHt          - Reference height for horizontal wind speed      (m)
        0.2   PLexp          - Power law exponent                              (-)
================== Parameters for Uniform wind file   [used only for WindType = 2] ============================
"Wind/90m_12mps_twr.hh"    FileName_Uni       - Filename of time series data for uniform wind field.      (-)
         90   RefHt_Uni      - Reference height for horizontal wind speed                (m)
     125.88   RefLength      - Reference length for linear horizontal and vertical sheer (-)
================== Parameters for Binary TurbSim Full-Field files   [used only for WindType = 3] ==============
"Wind/90m_12mps_twr.bts"    Filename       - Name of the Full field wind file to use (.bts)
================== Parameters for Binary Bladed-style Full-Field files   [used only for WindType = 4 or WindType = 7] =========
"Wind/90m_12mps_twr"    FilenameRoot   - WindType=4: Rootname of the full-field wind file to use (.wnd, .sum); WindType=7: name of the intermediate file with wind scaling values
False         TowerFile      - Have tower file (.twr) (flag) ignored when WindType = 7
================== Parameters for HAWC-format binary files  [Only used with WindType = 5] =====================
"wasp\Output\basic_5u.bin"    FileName_u     - name of the file containing the u-component fluctuating wind (.bin)
"wasp\Output\basic_5v.bin"    FileName_v     - name of the file containing the v-component fluctuating wind (.bin)
"wasp\Output\basic_5w.bin"    FileName_w     - name of the file containing the w-component fluctuating wind (.bin)
         64   nx             - number of grids in the x direction (in the 3 files above) (-)
         32   ny             - number of grids in the y direction (in the 3 files above) (-)
         32   nz             - number of grids in the z direction (in the 3 files above) (-)
         16   dx             - distance (in meters) between points in the x direction    (m)
          3   dy             - distance (in meters) between points in the y direction    (m)
          3   dz             - distance (in meters) between points in the z direction    (m)
         90   RefHt_HAWC     - reference height; the height (in meters) of the vertical center of the grid (m)
  -------------   Scaling parameters for turbulence   ---------------------------------------------------------
          2   ScaleMethod    - Turbulence scaling method   [0 = none, 1 = direct scaling, 2 = calculate scaling factor based on a desired standard deviation]
          1   SFx            - Turbulence scaling factor for the x direction (-)   [ScaleMethod=1]
          1   SFy            - Turbulence scaling factor for the y direction (-)   [ScaleMethod=1]
          1   SFz            - Turbulence scaling factor for the z direction (-)   [ScaleMethod=1]
        1.2   SigmaFx        - Turbulence standard deviation to calculate scaling from in x direction (m/s)    [ScaleMethod=2]
         .8   SigmaFy        - Turbulence standard deviation to calculate scaling from in y direction (m/s)    [ScaleMethod=2]
         .2   SigmaFz        - Turbulence standard deviation to calculate scaling from in z direction (m/s)    [ScaleMethod=2]
  -------------   Mean wind profile parameters (added to HAWC-format files)   ---------------------------------
         12   URef           - Mean u-component wind speed at the reference height (m/s)
          2   WindProfile    - Wind profile type (0=constant;1=logarithmic,2=power law)
        0.2   PLExp_HAWC     - Power law exponent (-) (used for PL wind profile type only)
       0.03   Z0             - Surface roughness length (m) (used for LG wind profile type only)
          0   XOffset        - Initial offset in +x direction (shift of wind box)
================== LIDAR Parameters ===========================================================================
          0   SensorType          - Switch for lidar configuration (0 = None, 1 = Single Point Beam(s), 2 = Continuous, 3 = Pulsed)
          0   NumPulseGate        - Number of lidar measurement gates (used when SensorType = 3)
         30   PulseSpacing        - Distance between range gates (m) (used when SensorType = 3)
          0   NumBeam             - Number of lidar measurement beams (0-5)(used when SensorType = 1)
       -200   FocalDistanceX      - Focal distance co-ordinates of the lidar beam in the x direction (relative to hub height) (only first coordinate used for SensorType 2 and 3) (m)
          0   FocalDistanceY      - Focal distance co-ordinates of the lidar beam in the y direction (relative to hub height) (only first coordinate used for SensorType 2 and 3) (m)
          0   FocalDistanceZ      - Focal distance co-ordinates of the lidar beam in the z direction (relative to hub height) (only first coordinate used for SensorType 2 and 3) (m)
0.0 0.0 0.0   RotorApexOffsetPos  - Offset of the lidar from hub height (m)
         17   URefLid             - Reference average wind speed for the lidar[m/s]
       0.25   MeasurementInterval - Time between each measurement [s]
      False   LidRadialVel        - TRUE => return radial component, FALSE => return 'x' direction estimate
          1   ConsiderHubMotion   - Flag whether to consider the hub motion's impact on Lidar measurements
====================== OUTPUT ==================================================
False         SumPrint     - Print summary data to <RootName>.IfW.sum (flag)
              OutList      - The next line(s) contains a list of output parameters.  See OutListParameters.xlsx for a listing of available output channels, (-)
"Wind1VelX"               X-direction wind velocity at point WindList(1)
"Wind1VelY"               Y-direction wind velocity at point WindList(1)
"Wind1VelZ"               Z-direction wind velocity at point WindList(1)
END of input file (the word "END" must appear in the first 3 columns of this last OutList line)
---------------------------------------------------------------------------------------
