# UTE PKDD-8
This markdown includes Chinese version and English version.

## Chinese
当前站点数据集仅公开部分sample样例数据。
pixel.csv文件中数据格式为[MOT15标准](https://motchallenge.net/instructions/)

### 采集路段
<b>采集地点经纬度：</b>32.062378,118.657484<br>

<b>路段类型：</b>平直道路<br>

<b>路段长度：</b>280m<br>

<b>路段限速：</b>80km/h<br>

<b>路段线形：</b>研究路段长度280米，西北-东南走向。双向八车道。

### 拍摄情况
<b>拍摄高度：</b>200m<br>

<b>采集日期：</b><br>

<b>采集时刻：</b>8:00<br>

<b>视频时长：</b>17m45s<br>

<b>视频帧率：</b>30<br>

### 交通信息
<b>交通状况：</b>自由流<br>

<b>轨迹数量：</b>1477<br>

<b>数据信息：</b>时间精度0.03s(fps30)，轨迹数量1477条。包含时间、车辆位置、车道、运动学等信息。<br>

### 下载链接
点此下载数据集[PKDD-8](https://pan.baidu.com/s/18DON_M3n2KHsQTzc1nkNKA?pwd=ttkp)


## English
The PKDD dataset only discloses sample data currently.
The data format in the pixel.csv file is [MOT15 standard](https://motchallenge.net/instructions/)

### road section
<b>Longitude and latitude：</b>32.062378,118.657484<br>

<b>section type：</b>straight section<br>

<b>section length：</b>280m<br>

<b>speed limit：</b>80km/h<br>

<b>section alignment：</b>The research section is 280 meters long, with a northwest-southeast direction. It has 8 lanes in both directions.

### shooting situation
<b>shooting height：</b>200m<br>

<b>shooting date：</b><br>

<b>shooting time：</b>8:00<br>

<b>video duraiton：</b>17m45s<br>

<b>frame rate：</b>30<br>

### traffic information
<b>traffic status：</b>free flow<br>

<b>number of trajectories：</b>1477<br>

<b>data profile：</b>The temporal accuracy is 0.03s (fps: 30), with 1477 number of tracks. It includes information on time, vehicle position, lane, kinematics, and more.<br>

### download
click here to download [PKDD-8](https://drive.google.com/drive/folders/1L6JNekxQ2-DTu82Suo6rEal3On-0JO-f?usp=sharing)


