Example Description

This example describes how to use ADC normal channel in auto mode.
In automatic mode, ADC would continuously execute conversions without any trigger sources after automatic channel switch register is set. 
Automatic mode would not stop conversions until the automatic channel switch is disable.




