This demo is used to decode JPG file and display on 16bit RGB I/F LCD. Follow these steps:
	1. Replace the original src folder with this src folder.
	2. Build and download images. 
	3. Download test.jpg to 0x08106000.
	4. Reset device and you will see the JPG picture display on LCD.
	