Example Description

This example rx music by AMIC2 and stream it out.

How to build:
	1. copy main.c and main.h to project\realtek_amebaD_va0_example\src\src_hp

Requirement Components:
    AmebaD_QFN88_EVB_V2

Set-up:
	1. Ensure J19 and J23 are each shorted(PIN2 and PIN3 should be shorted) respectively with jumpers.
	2. Ensure J21 is shorted(PIN2 and PIN3 should be shorted) with jumpers.
	3. Ensure JP12 is shorted with jumpers.
	4. Plug in earphone/speaker into JACK(CTIA).
	5. Ensure J18 and J22 are each shorted(PIN1 and PIN2 should be shorted) respectively with jumpers.

Behavior:
	Listen to audio output from speaker jack.

Note:
	If you want to play PC music connect to board, please change the jumpers.
		1. Ensure J19 and J23 are each shorted(PIN1 and PIN2 should be shorted) respectively with jumpers.
		2. Ensure J21 is shorted(PIN1 and PIN2 should be shorted) with jumpers.

