Example Description

This example describes how to use GDMA's single-block transfer mode with Mbed API.

How to build:
	1. copy main.c to project\realtek_amebaD_va0_example\src\src_hp

Requirement Components:
    None

Behaviour:
	GDMA will display below log in serial port tool.
	"DMA Copy Done!!
	 DMA Copy Memory Compare OK!! ff"

