Example Description

This example rx sound by DMIC and stream it out.

How to build:
	1. copy main.c and main.h to project\realtek_amebaD_va0_example\src\src_hp

Requirement Components:
    AmebaD_QFN88_EVB_V2

Set-up:
	1. Ensure J14 and J15 are each shorted respectively with jumpers.
	2. Plug in earphone/speaker into JACK(CTIA).
	3. Ensure J18 and J22 are each shorted(PIN1 and PIN2 should be shorted) respectively with jumpers.

Behavior:
	Listen to audio output from speaker jack.

