Example Description

This example describes how to use Timer5 input capture function.

Requirement Components:
    None

Behaviour:
- PA_13 as TIM5 PWM channel output 32K, connect it to PB_5
- PB_5 as TIM5 input capture pin. 

This example will print out the frequency of pwm captured.
 