Configuration Name: HOSTMOT2

General configuration information:

  BoardName : MESA7C80
  FPGA Size: 9 KGates
  FPGA Pins: 144
  Number of IO Ports: 2
  Width of one I/O port: 27
  Clock Low frequency: 100.0000 MHz
  Clock High frequency: 200.0000 MHz
  IDROM Type: 3
  Instance Stride 0: 4
  Instance Stride 1: 64
  Register Stride 0: 256
  Register Stride 1: 256

Modules in configuration:

  Module: DPLL
  There are 1 of DPLL in configuration
  Version: 0
  Registers: 7
  BaseAddress: 7000
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: WatchDog
  There are 1 of WatchDog in configuration
  Version: 0
  Registers: 3
  BaseAddress: 0C00
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: IOPort
  There are 2 of IOPort in configuration
  Version: 0
  Registers: 5
  BaseAddress: 1000
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: QCount
  There are 2 of QCount in configuration
  Version: 2
  Registers: 5
  BaseAddress: 3000
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: StepGen
  There are 9 of StepGen in configuration
  Version: 2
  Registers: 10
  BaseAddress: 2000
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: SSerial
  There are 1 of SSerial in configuration
  Version: 0
  Registers: 6
  BaseAddress: 5B00
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 64 bytes

  Module: PWM
  There are 2 of PWM in configuration
  Version: 0
  Registers: 5
  BaseAddress: 4100
  ClockFrequency: 200.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: SSR
  There are 1 of SSR in configuration
  Version: 0
  Registers: 2
  BaseAddress: 7D00
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: InMux
  There are 1 of InMux in configuration
  Version: 0
  Registers: 5
  BaseAddress: 8000
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

  Module: LED
  There are 1 of LED in configuration
  Version: 0
  Registers: 1
  BaseAddress: 0200
  ClockFrequency: 100.000 MHz
  Register Stride: 256 bytes
  Instance Stride: 4 bytes

Configuration pin-out:

IO Connections for StepGens+Misc
Pin#  I/O   Pri. func    Sec. func       Chan      Pin func        Pin Dir

 0      0   IOPort       StepGen          0        Step/Table1     (Out)
 0      1   IOPort       StepGen          0        Dir/Table2      (Out)
 0      2   IOPort       StepGen          1        Step/Table1     (Out)
 0      3   IOPort       StepGen          1        Dir/Table2      (Out)
 0      4   IOPort       StepGen          2        Step/Table1     (Out)
 0      5   IOPort       StepGen          2        Dir/Table2      (Out)
 0      6   IOPort       StepGen          3        Step/Table1     (Out)
 0      7   IOPort       StepGen          3        Dir/Table2      (Out)
 0      8   IOPort       StepGen          4        Step/Table1     (Out)
 0      9   IOPort       StepGen          4        Dir/Table2      (Out)
 0     10   IOPort       StepGen          5        Step/Table1     (Out)
 0     11   IOPort       StepGen          5        Dir/Table2      (Out)
 0     12   IOPort       SSerial          0        RXData0         (In)
 0     13   IOPort       SSerial          0        TXData0         (Out)
 0     14   IOPort       SSerial          0        TXEn0           (Out)
 0     15   IOPort       QCount           0        Quad-A          (In)
 0     16   IOPort       QCount           0        Quad-B          (In)
 0     17   IOPort       QCount           0        Quad-IDX        (In)
 0     18   IOPort       PWM              0        PWM             (Out)
 0     19   IOPort       PWM              0        /Enable         (Out)
 0     20   IOPort       None           
 0     21   IOPort       None           
 0     22   IOPort       InMux            0        Addr0           (Out)
 0     23   IOPort       InMux            0        Addr1           (Out)
 0     24   IOPort       InMux            0        Addr2           (Out)
 0     25   IOPort       InMux            0        Addr3           (Out)
 0     26   IOPort       InMux            0        Addr4           (Out)

IO Connections for Outputs+P1
Pin#  I/O   Pri. func    Sec. func       Chan      Pin func        Pin Dir

 0     27   IOPort       InMux            0        Data0           (In)
 0     28   IOPort       SSR              0        Out-00          (Out)
 0     29   IOPort       SSR              0        Out-01          (Out)
 0     30   IOPort       SSR              0        Out-02          (Out)
 0     31   IOPort       SSR              0        Out-03          (Out)
 0     32   IOPort       SSR              0        Out-04          (Out)
 0     33   IOPort       SSR              0        Out-05          (Out)
 0     34   IOPort       SSR              0        Out-06          (Out)
 0     35   IOPort       SSR              0        Out-07          (Out)
 0     36   IOPort       SSR              0        AC Ref          (Out)
 0     37   IOPort       PWM              1        PWM             (Out)
 0     38   IOPort       None           
 0     39   IOPort       StepGen          6        Step/Table1     (Out)
 0     40   IOPort       None           
 0     41   IOPort       StepGen          6        Dir/Table2      (Out)
 0     42   IOPort       None           
 0     43   IOPort       StepGen          7        Step/Table1     (Out)
 0     44   IOPort       None           
 0     45   IOPort       StepGen          7        Dir/Table2      (Out)
 0     46   IOPort       StepGen          8        Step/Table1     (Out)
 0     47   IOPort       StepGen          8        Dir/Table2      (Out)
 0     48   IOPort       None           
 0     49   IOPort       None           
 0     50   IOPort       None           
 0     51   IOPort       QCount           1        Quad-A          (In)
 0     52   IOPort       QCount           1        Quad-B          (In)
 0     53   IOPort       QCount           1        Quad-IDX        (In)

