## Assembly Guidelines of the HackberryPi_CM5

Assembly is straightforward: install the CM5 module, secure the heat sink,, here are the steps for the assembly


### Firstly, disassemble the back plate with the screw driver in the box
![image](https://github.com/user-attachments/assets/7b104ea4-0e25-42a2-87a7-8331de99e380)

### Secondly put the Compute module5 on the slot 
![image](https://github.com/user-attachments/assets/3bb29381-14d2-434d-a372-9b2b1c0e18c4)

### Then use the white printed tool to secure the yellow screws
![image](https://github.com/user-attachments/assets/d07a4d60-4d26-4206-b65e-26ac93872374)
![image](https://github.com/user-attachments/assets/1803a0f1-7f5d-47a9-a144-54577faf5720)

### Don't forget this: Place the thermal silicone pad onto the CM5 module.
![image](https://github.com/user-attachments/assets/d82e1700-abcb-462e-9333-f6410813fed2)

### At last secure the heat sink with screws and lock the back plate.
![image](https://github.com/user-attachments/assets/650cfd96-d7de-4a42-bbd4-cd2389b7efec)
![image](https://github.com/user-attachments/assets/2c8f3c18-104d-44b0-bcc3-6b6f5a593201)

Now it's OK to turn on the device and enjoy your time with it!!!
