&eeprom0 {
	nvmem-layout {
		compatible = "fixed-layout";
		#address-cells = <1>;
		#size-cells = <1>;

		mac_address: mac_address@0 {
			reg = <0x0 6>;
			#nvmem-cell-cells = <0>;
			read-only;
		};

		calibration_data: calibration_data@6 {
			reg = <0x6 100>;
			#nvmem-cell-cells = <0>;
		};
	};
};
