.. zephyr:board:: esp32s3_touch_lcd_1_28

Overview
********

The ESP32-S3-Touch-LCD-1.28 is an ESP32S3 development board from Waveshare with a round LCD,
suitable to build watches or similar projects. This board integrates complete Wi-Fi and Bluetooth
Low Energy functions, an accelerometer and gyroscope, a battery charger and GPIO extension port.

Hardware
********

.. include:: ../../../espressif/common/soc-esp32s3-features.rst
   :start-after: espressif-soc-esp32s3-features

Supported Features
==================

.. zephyr:board-supported-hw::

System Requirements
*******************

.. include:: ../../../espressif/common/system-requirements.rst
   :start-after: espressif-system-requirements

Programming and Debugging
*************************

.. zephyr:board-supported-runners::

.. include:: ../../../espressif/common/building-flashing.rst
   :start-after: espressif-building-flashing

.. include:: ../../../espressif/common/board-variants.rst
   :start-after: espressif-board-variants

Debugging
=========

.. include:: ../../../espressif/common/openocd-debugging.rst
   :start-after: espressif-openocd-debugging

References
**********

.. target-notes::

.. _`ESP32-S3-Touch-LCD-1.28 Waveshare Wiki`: https://www.waveshare.com/wiki/ESP32-S3-Touch-LCD-1.28
