.. zephyr:board:: thingy53

Overview
********

Zephyr uses the ``thingy53/nrf5340`` board configuration for building
for the Thingy:53 board. The board has the nRF5340 MCU processor, a set of
environmental sensors, a pushbutton, and RGB LED.

The nRF5340 is a dual-core SoC based on the Arm® Cortex®-M33 architecture, with:

* a full-featured Arm Cortex-M33F core with DSP instructions, FPU, and
  Armv8-M Security Extension, running at up to 128 MHz, referred to as
  the **application core**
* a secondary Arm Cortex-M33 core, with a reduced feature set, running at
  a fixed 64 MHz, referred to as the **network core**.

The ``thingy53/nrf5340/cpuapp`` build target provides support for the application
core on the nRF5340 SoC. The ``thingy53/nrf5340/cpunet`` build target provides
support for the network core on the nRF5340 SoC.

The `Nordic Thingy:53 Hardware guide`_ contains the processor's information and
the datasheet.

Hardware
********

Supported Features
==================

.. zephyr:board-supported-hw::

Programming and Debugging
*************************

.. zephyr:board-supported-runners::

Flashing
========

Flashing Zephyr onto Thingy:53 requires an external J-Link programmer. The
programmer is attached to the P9 programming header.

Debugging
=========

Thingy:53 does not have an on-board J-Link debug IC as some other nRF5
development boards, however, instructions from the :ref:`nordic_segger` page
also apply to this board, with the additional step of connecting an external
debugger. A development board with a Debug out connector such as the
:zephyr:board:`nrf5340dk` can be used as a debugger with Thingy:53.

References
**********

.. target-notes::

.. _Nordic Thingy:53 Hardware guide: https://docs.nordicsemi.com/bundle/ug_thingy53/page/UG/thingy53/intro/frontpage.html
