.. zephyr:board:: esp32c3_supermini

Overview
********

ESP32-C3-SUPERMINI is based on the ESP32-C3, a single-core Wi-Fi and Bluetooth 5 (LE) microcontroller SoC,
based on the open-source RISC-V architecture. This board also includes a Type-C USB Serial/JTAG port.
There may be multiple variations depending on the specific vendor.
For more information a reasonably well documented version of this board can be found at `ESP32-C3-SUPERMINI`_

Hardware
********

.. include:: ../../../espressif/common/soc-esp32c3-features.rst
   :start-after: espressif-soc-esp32c3-features

Supported Features
==================

.. zephyr:board-supported-hw::

System Requirements
*******************

.. include:: ../../../espressif/common/system-requirements.rst
   :start-after: espressif-system-requirements

Programming and Debugging
*************************

.. zephyr:board-supported-runners::

.. include:: ../../../espressif/common/building-flashing.rst
   :start-after: espressif-building-flashing

.. include:: ../../../espressif/common/board-variants.rst
   :start-after: espressif-board-variants

Debugging
=========

.. include:: ../../../espressif/common/openocd-debugging.rst
   :start-after: espressif-openocd-debugging

References
**********

.. target-notes::

.. _`ESP32-C3-SUPERMINI`: https://www.nologo.tech/product/esp32/esp32c3SuperMini/esp32C3SuperMini.html
