.. zephyr:board:: particle_argon

Overview
********

The Particle Argon is a Wi-Fi enabled development board with a Nordic
Semiconductor nRF52840 for mesh support and an ESP32 for Wi-Fi.  The
board was developed by Particle Industries and has a SWD connector on it
for programming.

It is equipped with a onboard LIPO circuit and conforms to the
Adafruit Feather formfactor.

The Particle Argon provides support for the Nordic Semiconductor nRF52840 ARM
|reg| Cortex |reg|-M4F SoC with an integrated 2.4 GHz transceiver supporting
Bluetooth |reg| Low Energy and IEEE |reg| 802.15.4.

For more information about the Particle Argon board:

- `Argon Datasheet`_
- `Argon Hardware Files`_

Hardware
********

On the front of the board are RGB-LED, LED and LIPO circuitry.
The RGB-LED is controlled by the nRF52840 via GPIO pins.

Power supply
============

The board is optimized for low power applications and supports two
power source configurations: battery and micro USB connector.

It contains circuitry for LIPO usage and can be charged via the USB port.

Supported Features
==================

.. zephyr:board-supported-hw::

Connections and IOs
===================

Please see the `Argon Datasheet`_ for header pin assignments, which are
common to all Feather-compatible Particle boards.  Some peripherals are
available to applications through DTS overlay include directives:

- ``mesh_feather_i2c1_twi1.dtsi`` exposes TWI1 on labeled Feather
  SDA1/SCL1 pins
- ``mesh_feather_spi_spi1.dtsi`` exposes SPI1 on labeled Feather
  SPI pins
- ``mesh_feather_spi_spi3.dtsi`` exposes SPI3 on labeled Feather
  SPI pins
- ``mesh_feather_spi1_spi3.dtsi`` exposes SPI3 on labeled Feather
  SPI1 pins
- ``mesh_feather_uart1_rtscts.dtsi`` adds hardware flow control to
  labeled Feather UART pins

LED
---

* LED0 (blue)
* LED1 (red)
* LED2 (green)
* LED3 (blue)

Push buttons
------------

* SW0 via MODE
* SW1 via RESET

I2C
---

* TWI0 enabled on labeled header (SDA/SCL)
* TWI1 selectable with overlay (SDA1/SCL1)

SPI
---

* SPI0 disabled due to TWI0 conflict
* SPI1 selectable with overlay (SPI)
* SPI2 internal to 32 Mb CFI flash chip
* SPI3 selectable with overlay (SPI or SPI1)

UART
----

* UARTE0 enabled RX/TX on labeled header (UART1); add RTS/CTS with overlay
* UARTE1 internal to ESP32

Programming and Debugging
*************************

.. zephyr:board-supported-runners::

Applications for the ``particle_argon`` board configuration can be
built and flashed in the usual way (see :ref:`build_an_application`
and :ref:`application_run` for more details).

Flashing
========

Build and flash an application in the usual way, for example:

.. zephyr-app-commands::
   :zephyr-app: samples/basic/blinky
   :board: particle_argon
   :goals: build flash

Debugging
=========

You can debug an application in the usual way.  Here is an example for the
:zephyr:code-sample:`hello_world` application.

.. zephyr-app-commands::
   :zephyr-app: samples/hello_world
   :board: particle_argon
   :maybe-skip-config:
   :goals: debug


Testing the LEDs and buttons
****************************

There are 2 samples that allow you to test that the buttons (switches) and
LEDs on the board are working properly with Zephyr:

* :zephyr:code-sample:`blinky`
* :zephyr:code-sample:`button`

You can build and flash the examples to make sure Zephyr is running correctly on
your board.

.. _Argon Datasheet:
   https://docs.particle.io/datasheets/wi-fi/argon-datasheet/

.. _Argon Hardware Files:
   https://github.com/particle-iot/argon
