.. zephyr:board:: we_proteus2ev

Overview
********

The Proteus-II-EV hardware provides
support for the Proteus-II radio module that uses the Nordic Semiconductor nRF52832 ARM Cortex-M4F CPU and
the following devices:

* :abbr:`ADC (Analog to Digital Converter)`
* CLOCK
* FLASH
* :abbr:`GPIO (General Purpose Input Output)`
* :abbr:`I2C (Inter-Integrated Circuit)`
* :abbr:`MPU (Memory Protection Unit)`
* :abbr:`NVIC (Nested Vectored Interrupt Controller)`
* :abbr:`PWM (Pulse Width Modulation)`
* RADIO (Bluetooth Low Energy)
* :abbr:`RTC (nRF RTC System Clock)`
* Segger RTT (RTT Console)
* :abbr:`SPI (Serial Peripheral Interface)`
* :abbr:`UART (Universal asynchronous receiver-transmitter)`
* :abbr:`WDT (Watchdog Timer)`

More information about the radio module can be found the Würth Elektronik web page https://www.we-online.com/katalog/de/PROTEUS-II .


Hardware
********

Proteus-II radio module provides only the internal oscillators. The frequency of the slow clock
is 32.768 kHz. The frequency of the main clock is 32 MHz.

Supported Features
==================

.. zephyr:board-supported-hw::

Connections and IOs
===================

LED
---

* LED1 = P0.00
* LED2 = P0.01

Push buttons
------------

* BUTTON1 = SW1 = P0.29


Programming and Debugging
*************************

.. zephyr:board-supported-runners::

Applications for the ``we_proteus2ev/nrf52832`` board configuration can be
built, flashed, and debugged in the usual way. See
:ref:`build_an_application` and :ref:`application_run` for more details on
building and running.

Flashing
========

Follow the instructions in the :ref:`nordic_segger` page to install
and configure all the necessary software. Further information can be
found in :ref:`nordic_segger_flashing`. Then build and flash
applications as usual (see :ref:`build_an_application` and
:ref:`application_run` for more details).

Here is an example for the :zephyr:code-sample:`hello_world` application.

First, run your favorite terminal program to listen for output.

.. code-block:: console

   $ minicom -D <tty_device> -b 115200

Replace :code:`<tty_device>` with the port where the board Proteus-II-EV
can be found. For example, under Linux, :code:`/dev/ttyACM0`.

Then build and flash the application in the usual way.

.. zephyr-app-commands::
   :zephyr-app: samples/hello_world
   :board: we_proteus2ev/nrf52832
   :goals: build flash

Debugging
=========

Refer to the :ref:`nordic_segger` page to learn about debugging Nordic boards with a
Segger IC.


Testing the LEDs and buttons in the Proteus-II-EV
*************************************************

There are 2 samples that allow you to test that the buttons (switches) and LEDs on
the board are working properly with Zephyr:

.. code-block:: console

   samples/basic/blinky
   samples/basic/button

You can build and flash the examples to make sure Zephyr is running correctly on
your board. The button and LED definitions can be found in
:zephyr_file:`boards/we/proteus2ev/we_proteus2ev_nrf52832.dts`.

References
**********

.. target-notes::

.. _Proteus-II radio module website: https://www.we-online.com/katalog/de/PROTEUS-II
.. _nRF52 DK website: https://www.nordicsemi.com/Software-and-Tools/Development-Kits/nRF52-DK
.. _Nordic Semiconductor Infocenter: https://infocenter.nordicsemi.com
