.. _eval_ad4052_ardz:

EVAL-AD4052-ARDZ
#################

Overview
********

The EVAL-AD4052-ARDZ is a 16-Bit SAR ADC Arduino shield powered
by the Analog Devices AD4052.

.. figure:: eval_ad4052_ardz.webp
   :align: center
   :alt: EVAL-AD4052-ARDZ

Programming
***********

Set ``--shield eval_ad4052_ardz`` when you invoke ``west build``. For example:

.. zephyr-app-commands::
   :zephyr-app: samples/drivers/adc/
   :board: apard32690/max32690/m4
   :shield: eval_ad4052_ardz
   :goals: build

Requirements
************

This shield can only be used with a board which provides a configuration for
Arduino connectors and defines node aliases for SPI and GPIO interfaces (see
:ref:`shields` for more details).

References
**********

- `EVAL-AD4052-ARDZ product page`_
- `EVAL-AD4052-ARDZ user guide`_
- `EVAL-AD4052-ARDZ schematic`_
- `AD4052 product page`_
- `AD4052 data sheet`_

.. _EVAL-AD4052-ARDZ product page:
   https://www.analog.com/en/resources/evaluation-hardware-and-software/evaluation-boards-kits/eval-ad4052-ardz.html#eb-overview

.. _EVAL-AD4052-ARDZ user guide:
   https://www.analog.com/media/en/technical-documentation/user-guides/eval-ad4050-ad4052-ug-2222.pdf

.. _EVAL-AD4052-ARDZ schematic:
   https://www.analog.com/media/en/evaluation-documentation/evaluation-design-files/eval-ad4052-ardz-designsupport-files.zip

.. _AD4052 product page:
   https://www.analog.com/en/products/ad4052.html

.. _AD4052 data sheet:
   https://www.analog.com/media/en/technical-documentation/data-sheets/ad4052-ad4058.pdf
