.. zephyr:board:: lpcxpresso55s28

Overview
********

The LPCXpresso55S28 development board provides the ideal platform for evaluation
of and development with the LPC552x/S2x MCU based on the Arm® Cortex®-M33
architecture. The board includes a high-performance onboard debug probe, audio
subsystem and accelerometer, with several options for adding off-the-shelf
add-on boards for networking, sensors, displays, and other interfaces.

Hardware
********

- LPC55S28 Arm® Cortex®-M33 microcontroller running at up to 150 MHz
- 512 KB flash and 256 KB SRAM on-chip
- Onboard, high-speed USB, Link2 debug probe with CMSIS-DAP and SEGGER J-Link
  protocol options
- UART and SPI port bridging from LPC55S28 target to USB via the onboard debug
  probe
- Hardware support for external debug probe
- 3 x user LEDs, plus Reset, ISP (3) and user buttons
- Micro SD card slot (4-bit SDIO)
- NXP MMA8652FCR1 accelerometer
- Stereo audio codec with line in/out
- High and full speed USB ports with micro A/B connector for host or device
  functionality
- MikroEletronika Click expansion option
- LPCXpresso-V3 expansion option compatible with Arduino UNO
- PMod compatible expansion / host connector

For more information about the LPC55S28 SoC and LPCXPresso55S28 board, see:

- `LPC55S28 SoC Website`_
- `LPC55S28 Datasheet`_
- `LPC55S28 User Manual`_
- `LPCXpresso55S28 Website`_
- `LPCXpresso55S28 User Manual`_
- `LPCXpresso55S28 Development Board Design Files`_

Supported Features
==================

.. zephyr:board-supported-hw::

.. note::

   For additional features not yet supported, please also refer to the
   :zephyr:board:`lpcxpresso55s69` , which is the superset board in NXP's LPC55xx series.
   NXP prioritizes enabling the superset board with NXP's Full Platform Support for
   Zephyr.  Therefore, the lpcxpresso55s69 board may have additional features
   already supported, which can also be re-used on this board.

Connections and IOs
===================

The LPC55S28 SoC has IOCON registers, which can be used to configure
the functionality of a pin.

+---------+-----------------+----------------------------+
| Name    | Function        | Usage                      |
+=========+=================+============================+
| PIO0_26 | SPI             | SPI MOSI                   |
+---------+-----------------+----------------------------+
| PIO0_29 | USART           | USART RX                   |
+---------+-----------------+----------------------------+
| PIO0_30 | USART           | USART TX                   |
+---------+-----------------+----------------------------+
| PIO1_1  | SPI             | SPI SSEL                   |
+---------+-----------------+----------------------------+
| PIO1_2  | SPI             | SPI SCK                    |
+---------+-----------------+----------------------------+
| PIO1_3  | SPI             | SPI MISO                   |
+---------+-----------------+----------------------------+
| PIO1_4  | GPIO            | RED LED                    |
+---------+-----------------+----------------------------+
| PIO1_6  | GPIO            | BLUE_LED                   |
+---------+-----------------+----------------------------+
| PIO1_7  | GPIO            | GREEN LED                  |
+---------+-----------------+----------------------------+
| PIO1_20 | I2C             | I2C SCL                    |
+---------+-----------------+----------------------------+
| PIO1_21 | I2C             | I2C SDA                    |
+---------+-----------------+----------------------------+

System Clock
============

The LPC55S28 SoC is configured to use PLL1 clocked from the external 24MHz
crystal, running at 144MHz as a source for the system clock. When the flash
controller is enabled, the core clock will be reduced to 96MHz. The application
may reconfigure clocks after initialization, provided that the core clock is
always set to 96MHz when flash programming operations are performed.

Serial Port
===========

The LPC55S28 SoC has 8 FLEXCOMM interfaces for serial communication. One is
configured as USART for the console and the remaining are not used.

Programming and Debugging
*************************

.. zephyr:board-supported-runners::

Build and flash applications as usual (see :ref:`build_an_application`
and :ref:`application_run` for more details).

Configuring a Debug Probe
=========================

LinkServer is the default runner for this board.
A debug probe is used for both flashing and debugging the board. This board is
configured by default to use the integrated :ref:`mcu-link-onboard-debug-probe`
in the CMSIS-DAP mode. To use this probe with Zephyr, you need to install the
:ref:`linkserver-debug-host-tools` and make sure they are in your search path.
Refer to the detailed overview about :ref:`application_debugging` for additional
information.

The integrated MCU-Link hardware can also be used as a J-Link probe with a
firmware update, as described in :ref:`mcu-link-jlink-onboard-debug-probe`.
The :ref:`jlink-debug-host-tools` should be available in this case.

Configuring a Console
=====================

Connect a USB cable from your PC to P6, and use the serial terminal of your
choice (minicom, putty, etc.) with the following settings:

- Speed: 115200
- Data: 8 bits
- Parity: None
- Stop bits: 1

Flashing
========

Here is an example for the :zephyr:code-sample:`hello_world` application.

.. zephyr-app-commands::
   :zephyr-app: samples/hello_world
   :board: lpcxpresso55s28
   :goals: flash

Open a serial terminal, reset the board (press the RESET button), and you should
see the following message in the terminal:

.. code-block:: console

   ***** Booting Zephyr OS v2.4.0 *****
   Hello World! lpcxpresso55s28

Debugging
=========

Here is an example for the :zephyr:code-sample:`hello_world` application.

.. zephyr-app-commands::
   :zephyr-app: samples/hello_world
   :board: lpcxpresso55s28
   :goals: debug

Open a serial terminal, step through the application in your debugger, and you
should see the following message in the terminal:

.. code-block:: console

   ***** Booting Zephyr OS zephyr-v2.4.0 *****
   Hello World! lpcxpresso55s28

.. include:: ../../common/board-footer.rst.inc

.. _LPC55S28 SoC Website:
   https://www.nxp.com/products/processors-and-microcontrollers/arm-microcontrollers/general-purpose-mcus/lpc5500-cortex-m33/lpc552x-s2x-mainstream-arm-cortex-m33-based-microcontroller-family:LPC552x-S2x

.. _LPC55S28 Datasheet:
   https://www.nxp.com/docs/en/nxp/data-sheets/LPC55S2x_LPC552x_DS.pdf

.. _LPC55S28 User Manual:
   https://www.nxp.com/webapp/Download?colCode=UM11126

.. _LPCxpresso55S28 Website:
   https://www.nxp.com/design/software/development-software/lpcxpresso55s28-development-board:LPC55S28-EVK

.. _LPCXpresso55S28 User Manual:
   https://www.nxp.com/webapp/Download?colCode=UM11158

.. _LPCXpresso55S28 Development Board Design Files:
   https://www.nxp.com/webapp/Download?colCode=LPCXpresso55S69-DS
