.. zephyr:board:: nucleo_u575zi_q

Overview
********

The Nucleo U575ZI Q board, featuring an ARM Cortex-M33 based STM32U575ZI MCU,
provides an affordable and flexible way for users to try out new concepts and
build prototypes by choosing from the various combinations of performance and
power consumption features. Here are some highlights of the Nucleo U575ZI Q
board:


- STM32U575ZI microcontroller in LQFP144 package
- Internal SMPS to generate V core logic supply
- Two types of extension resources:

  - Arduino Uno V3 connectivity
  - ST morpho extension pin headers for full access to all STM32 I/Os

- On-board ST-LINK/V3E debugger/programmer
- Flexible board power supply:

   - USB VBUS or external source(3.3V, 5V, 7 - 12V)
   - ST-Link V3E

- Three users LEDs
- Two push-buttons: USER and RESET
- USB Type-C |reg| Sink device FS

Hardware
********

The STM32U575xx devices are an ultra-low-power microcontrollers family (STM32U5
Series) based on the high-performance Arm |reg| Cortex |reg|-M33 32-bit RISC core.
They operate at a frequency of up to 160 MHz.

- Ultra-low-power with FlexPowerControl (down to 300 nA Standby mode and 19.5 uA/MHz run mode)
- Core: ARM |reg| 32-bit Cortex |reg| -M33 CPU with TrustZone |reg| and FPU.
- Performance benchmark:

  - 1.5 DMPIS/MHz (Drystone 2.1)
  - 651 CoreMark |reg| (4.07 CoreMark |reg| /MHZ)

- Security

  - Arm |reg|  TrustZone |reg| and securable I/Os memories and peripherals
  - Flexible life cycle scheme with RDP (readout protection) and password protected debug
  - Root of trust thanks to unique boot entry and secure hide protection area (HDP)
  - Secure Firmware Installation thanks to embedded Root Secure Services
  - Secure Firmware Update support with TF-M
  - HASH hardware accelerator
  - Active tampers
  - True Random Number Generator NIST SP800-90B compliant
  - 96-bit unique ID
  - 512-byte One-Time Programmable for user data

- Clock management:

  - 4 to 50 MHz crystal oscillator
  - 32 kHz crystal oscillator for RTC (LSE)
  - Internal 16 MHz factory-trimmed RC ( |plusminus| 1%)
  - Internal low-power 32 kHz RC ( |plusminus| 5%)
  - 2 internal multispeed 100 kHz to 48 MHz oscillators, including one auto-trimmed by
    LSE (better than  |plusminus| 0.25 % accuracy)
  - 3 PLLs for system clock, USB, audio, ADC
  - Internal 48 MHz with clock recovery

- Power management

  - Embedded regulator (LDO)
  - Embedded SMPS step-down converter supporting switch on-the-fly and voltage scaling

- RTC with HW calendar and calibration
- Up to 136 fast I/Os, most 5 V-tolerant, up to 14 I/Os with independent supply down to 1.08 V
- Up to 24 capacitive sensing channels: support touchkey, linear and rotary touch sensors
- Up to 17 timers and 2 watchdogs

  - 2x 16-bit advanced motor-control
  - 2x 32-bit and 5 x 16-bit general purpose
  - 4x low-power 16-bit timers (available in Stop mode)
  - 2x watchdogs
  - 2x SysTick timer

- ART accelerator

  - 8-Kbyte instruction cache allowing 0-wait-state execution from Flash and
    external memories: up to 160 MHz, MPU, 240 DMIPS and DSP
  - 4-Kbyte data cache for external memories

- Memories

  - 2-Mbyte Flash memory with ECC, 2 banks read-while-write, including 512 Kbytes with 100 kcycles
  - 786-Kbyte SRAM with ECC OFF or 722-Kbyte SRAM including up to 322-Kbyte SRAM with ECC ON
  - External memory interface supporting SRAM, PSRAM, NOR, NAND and FRAM memories
  - 2 Octo-SPI memory interfaces

- Rich analog peripherals (independent supply)

  - 14-bit ADC 2.5-Msps, resolution up to 16 bits with hardware oversampling
  - 12-bit ADC 2.5-Msps, with hardware oversampling, autonomous in Stop 2 mode
  - 2 12-bit DAC, low-power sample and hold
  - 2 operational amplifiers with built-in PGA
  - 2 ultra-low-power comparators

- Up to 22 communication interfaces

  - USB Type-C / USB power delivery controller
  - USB OTG 2.0 full-speed controller
  - 2x SAIs (serial audio interface)
  - 4x I2C FM+(1 Mbit/s), SMBus/PMBus
  - 6x USARTs (ISO 7816, LIN, IrDA, modem)
  - 3x SPIs (5x SPIs with dual OCTOSPI in SPI mode)
  - 1x FDCAN
  - 2x SDMMC interface
  - 16- and 4-channel DMA controllers, functional in Stop mode
  - 1 multi-function digital filter (6 filters)+ 1 audio digital filter with
    sound-activity detection

- CRC calculation unit
- Development support: serial wire debug (SWD), JTAG, Embedded Trace Macrocell |trade|
- True Random Number Generator (RNG)

- Graphic features

  - Chrom-ART Accelerator (DMA2D) for enhanced graphic content creation
  - 1 digital camera interface

- Mathematical co-processor

 - CORDIC for trigonometric functions acceleration
 - FMAC (filter mathematical accelerator)

More information about STM32U575ZI can be found here:

- `STM32U575ZI on www.st.com`_
- `STM32U575 reference manual`_

Supported Features
==================

.. zephyr:board-supported-hw::

Connections and IOs
===================

Nucleo U575ZI Q Board has 9 GPIO controllers. These controllers are responsible for pin muxing,
input/output, pull-up, etc.

For more details please refer to `STM32 Nucleo-144 board User Manual`_.

Default Zephyr Peripheral Mapping:
----------------------------------


- CAN/CANFD_TX: PD1
- CAN/CANFD_RX: PD0
- DAC1_OUT1 : PA4
- I2C_1_SCL : PB8
- I2C_1_SDA : PB9
- I2C_2_SCL : PF1
- I2C_2_SDA : PF0
- LD1 : PC7
- LD2 : PB7
- LD3 : PG2
- LPUART_1_TX : PG7
- LPUART_1_RX : PG8
- SPI_1_NSS : PA4
- SPI_1_SCK : PA5
- SPI_1_MISO : PA6
- SPI_1_MOSI : PA7
- UART_1_TX : PA9
- UART_1_RX : PA10
- UART_2_TX : PD5
- UART_2_RX : PD6
- USER_PB : PC13

System Clock
------------

Nucleo U575ZI Q System Clock could be driven by internal or external oscillator,
as well as main PLL clock. By default System clock is driven by PLL clock at
160MHz, driven by 4MHz medium speed internal oscillator.

Serial Port
-----------

Nucleo U575ZI Q board has 6 U(S)ARTs. The Zephyr console output is assigned to
USART1. Default settings are 115200 8N1.


Backup SRAM
-----------

In order to test backup SRAM you may want to disconnect VBAT from VDD. You can
do it by removing ``SB50`` jumper on the back side of the board.


Programming and Debugging
*************************

.. zephyr:board-supported-runners::

Nucleo U575ZI-Q board includes an ST-LINK/V3 embedded debug tool interface.
This probe allows to flash the board using various tools.

Flashing
========

The board is configured to be flashed using west `STM32CubeProgrammer`_ runner,
so its :ref:`installation <stm32cubeprog-flash-host-tools>` is required.

Alternatively, OpenOCD, JLink, or pyOCD can also be used to flash the board using
the ``--runner`` (or ``-r``) option:

.. code-block:: console

   $ west flash --runner openocd
   $ west flash --runner jlink
   $ west flash --runner pyocd

For pyOCD, additional target information needs to be installed.
This can be done by executing the following commands.

.. code-block:: console

   $ pyocd pack --update
   $ pyocd pack --install stm32u5


Flashing an application to Nucleo U575ZI Q
------------------------------------------

Connect the Nucleo U575ZI Q to your host computer using the USB port.
Then build and flash an application. Here is an example for the
:zephyr:code-sample:`hello_world` application.

Run a serial host program to connect with your Nucleo board:

.. code-block:: console

   $ minicom -D /dev/ttyACM0

Then build and flash the application.

.. zephyr-app-commands::
   :zephyr-app: samples/hello_world
   :board: nucleo_u575zi_q
   :goals: build flash

You should see the following message on the console:

.. code-block:: console

   Hello World! arm

Debugging
=========

Default flasher for this board is openocd. It could be used in the usual way.
Here is an example for the :zephyr:code-sample:`blinky` application.

.. zephyr-app-commands::
   :zephyr-app: samples/basic/blinky
   :board: nucleo_u575zi_q
   :goals: debug

.. _STM32 Nucleo-144 board User Manual:
   https://www.st.com/resource/en/user_manual/dm00615305.pdf

.. _STM32U575ZI on www.st.com:
   https://www.st.com/en/microcontrollers/stm32u575zi.html

.. _STM32U575 reference manual:
   https://www.st.com/resource/en/reference_manual/rm0456-stm32u575585-armbased-32bit-mcus-stmicroelectronics.pdf

.. _STM32CubeProgrammer:
   https://www.st.com/en/development-tools/stm32cubeprog.html

.. _STMicroelectronics customized version of OpenOCD:
   https://github.com/STMicroelectronics/OpenOCD
