.. zephyr:board:: raytac_mdbt50q_db_40

Overview
********

The Raytac MDBT50Q-DB-40 hardware provides support for the
Nordic Semiconductor nRF52840 ARM Cortex-M4F CPU and the following devices:

* :abbr:`ADC (Analog to Digital Converter)`
* CLOCK
* FLASH
* :abbr:`GPIO (General Purpose Input Output)`
* :abbr:`I2C (Inter-Integrated Circuit)`
* :abbr:`MPU (Memory Protection Unit)`
* :abbr:`NVIC (Nested Vectored Interrupt Controller)`
* :abbr:`PWM (Pulse Width Modulation)`
* RADIO (Bluetooth Low Energy and 802.15.4)
* :abbr:`RTC (nRF RTC System Clock)`
* Segger RTT (RTT Console)
* :abbr:`SPI (Serial Peripheral Interface)`
* :abbr:`UART (Universal asynchronous receiver-transmitter)`
* :abbr:`USB (Universal Serial Bus)`
* :abbr:`WDT (Watchdog Timer)`

More information about the board can be found at the `MDBT50Q-DB-40 website`_.
The `MDBT50Q-DB-40 Specification`_ contains the demo board's datasheet.
The `MDBT50Q-DB-40 Schematic`_ contains the demo board's schematic.

Hardware
********
- Module Demo Board build by MDBT50Q-1MV2
- Nordic nRF52840 SoC Solution Version: 2
- A recommended 3rd-party module by Nordic Semiconductor.
- BT5.2&BT5.1&BT5 Bluetooth Specification Certified
- Supports BT5 Long Range Features
- Certifications: FCC, IC, CE, Telec(MIC), KC, SRRC, NCC, RCM, WPC
- 32-bit ARM® Cortex |reg| M4F CPU
- 1MB Flash Memory/256kB RAM
- RoHs & Reach Compliant.
- 48 GPIO
- Chip Antenna
- Interfaces: SPI, UART, I2C, I2S, PWM, ADC, NFC, and USB
- Highly flexible multiprotocol SoC ideally suited for Bluetooth® Low Energy, ANT+, Zigbee, Thread (802.15.4) ultra low-power wireless applications.
- 3 User LEDs
- 4 User buttons
- 1 Mini USB connector for power supply and USB communication
- SWD connector for FW programming
- J-Link interface for FW programming
- UART interface for UART communication

Supported Features
==================

.. zephyr:board-supported-hw::

See `MDBT50Q-DB-40 website`_ and `MDBT50Q-DB-40 Specification`_
for a complete list of Raytac MDBT50Q-DB-40 board hardware features.

Connections and IOs
===================

LED
---

* LED1 (green) = P0.13
* LED2 (red) = P0.14
* LED3 (blue) = P0.15

Push buttons
------------

* BUTTON1 = SW1 = P0.11
* BUTTON2 = SW2 = P0.12
* BUTTON3 = SW3 = P0.24
* BUTTON4 = SW4 = P0.25

UART
----
* RXD = P0.08
* TXD = P0.06
* RTS = P0.05
* CTS = P0.07

Programming and Debugging
*************************

.. zephyr:board-supported-runners::

Applications for the ``raytac_mdbt50q_db_40/nrf52840`` board configuration can be
built, flashed, and debugged in the usual way. See :ref:`build_an_application` and
:ref:`application_run` for more details on building and running.

.. note::
   Flashing and Debugging Zephyr onto the raytac_mdbt50q_db_40/nrf52840 board
   requires an	external J-Link programmer. The programmer is attached to the J1
   or J9 SWD connector.

Flashing
========

Follow the instructions in the :ref:`nordic_segger` page to install
and configure all the necessary software. Further information can be
found in :ref:`nordic_segger_flashing`. Then build and flash
applications as usual (see :ref:`build_an_application` and
:ref:`application_run` for more details).

Here is an example for the :zephyr:code-sample:`hello_world` application.

Use a USB to TTL converter to connect the computer and raytac_mdbt50q_db_40/nrf52840
J10 connector. Then run your favorite terminal program to listen for output.

.. code-block:: console

   $ minicom -D <tty_device> -b 115200

Replace :code:`<tty_device>` with the port where the USB to TTL converter
can be found. For example, under Linux, :code:`/dev/ttyUSB0`.

Then build and flash the application in the usual way.

.. zephyr-app-commands::
   :zephyr-app: samples/hello_world
   :board: raytac_mdbt50q_db_40/nrf52840
   :goals: build flash

Debugging
=========

The ``raytac_mdbt50q_db_40/nrf52840`` board does not have an on-board-J-Link debug IC,
however, instructions from the :ref:`nordic_segger` page also apply to this board.
Use the Debug out connector of nRF52x DK to connect to the J1 connector, and use SEGGER
J-Link OB IF to debug.

Testing the LEDs and buttons in the MDBT50Q-DB-40
*************************************************

There are 2 samples that allow you to test that the buttons (switches) and LEDs on
the board are working properly with Zephyr:

.. code-block:: console

   samples/basic/blinky
   samples/basic/button

You can build and flash the examples to make sure Zephyr is running correctly on
your board. The button and LED definitions can be found in
:zephyr_file:`boards/raytac/mdbt50q_db_40/raytac_mdbt50q_db_40_nrf52840.dts`.

Selecting the pins
==================

Pins can be configured in the board pinctrl file. To see the available mappings,
open the `MDBT50Q-DB-40 Specification`_, chapter 2.5 'Pin Assignment'.
Select the pins marked 'General-purpose I/O'. Note that pins marked as 'low-frequency I/O
only' can only be used in under-10KHz applications. They are not suitable for SPI, I2C,
UART, and PWM.

References
**********

.. target-notes::

.. _MDBT50Q-DB-40 website:
	https://www.raytac.com/product/ins.php?index_id=81
.. _MDBT50Q-DB-40 Specification:
	https://www.raytac.com/download/index.php?index_id=43
.. _MDBT50Q-DB-40 Schematic:
	https://www.raytac.com/upload/catalog_b/134ade06b5db3dd5803d27c5b17f22f3.jpg
.. _J-Link Software and documentation pack:
	https://www.segger.com/jlink-software.html
