.. zephyr:board:: adafruit_itsybitsy_m4_express

Overview
********

The Adafruit ItsyBitsy M4 express is a small (36 mm x 18 mm) ARM development
board with an onboard RGB LED, USB port, 2 MiB of SPI flash, and range of I/O
broken out onto 23 GPIO pins.

Hardware
********

- ATSAMD51G19A ARM Cortex-M4 processor at 120 MHz
- 512 KiB of flash memory and 192 KiB of RAM
- 2 MiB of SPI flash
- Internal trimmed 8 MHz oscillator
- A user LED
- An RGB DotStar LED
- Native USB port
- One reset button

Supported Features
==================

.. zephyr:board-supported-hw::

Zephyr can use the default Cortex-M SYSTICK timer or the SAM0 specific RTC.
To use the RTC, set :code:`CONFIG_CORTEX_M_SYSTICK=n` and set
:code:`CONFIG_SYS_CLOCK_TICKS_PER_SEC` to no more than 32 kHZ divided by 7,
i.e. no more than 4500.

Connections and IOs
===================

The `Adafruit Learning System`_ has detailed information about
the board including `pinouts`_ and the `schematic`_.

System Clock
============

The SAMD51 MCU is configured to use the 32 kHz internal oscillator
with the on-chip PLL generating the 120 MHz system clock.

Serial Port
===========

The SAMD51 MCU has 6 SERCOM based USARTs.  On the ItsyBitsy, SERCOM3 is
the Zephyr console and is available on pins 0 (RX) and 1 (TX).

SPI Port
========

The SAMD51 MCU has 6 SERCOM based SPIs.  On the ItsyBitsy, SERCOM1 can be put
into SPI mode and used to connect to devices over the SCK (SCLK), MO (MOSI), and
MI (MISO) pins.

PWM
===

The SAMD51 has three PWM generators with up to six channels each.  :code:`TCC_0`
has a resolution of 24 bits and all other generators are 16 bit.  :code:`TCC_1`
pin 2 is mapped to PA18 (D7) and pin 3 is mapped to PA19 (D9).

USB Device Port
===============

The SAMD51 MCU has a USB device port that can be used to communicate
with a host PC.  See the :zephyr:code-sample-category:`usb` sample applications for
more, such as the :zephyr:code-sample:`usb-cdc-acm` sample which sets up a virtual
serial port that echos characters back to the host PC.

Programming and Debugging
*************************

.. zephyr:board-supported-runners::

The ItsyBitsy ships with a the BOSSA compatible UF2 bootloader.  The
bootloader can be entered by quickly tapping the reset button twice.

Additionally, if :code:`CONFIG_USB_CDC_ACM` is enabled then the bootloader
will be entered automatically when you run :code:`west flash`.

Flashing
========

#. Build the Zephyr kernel and the :zephyr:code-sample:`hello_world` sample application:

   .. zephyr-app-commands::
      :zephyr-app: samples/hello_world
      :board: adafruit_itsybitsy_m4_express
      :goals: build
      :compact:

#. Connect the ItsyBitsy to your host computer using USB

#. Connect a 3.3 V USB to serial adapter to the board and to the
   host.  See the `Serial Port`_ section above for the board's pin
   connections.

#. Run your favorite terminal program to listen for output. Under Linux the
   terminal should be :code:`/dev/ttyUSB0`. For example:

   .. code-block:: console

      $ minicom -D /dev/ttyUSB0 -o

   The -o option tells minicom not to send the modem initialization
   string. Connection should be configured as follows:

   - Speed: 115200
   - Data: 8 bits
   - Parity: None
   - Stop bits: 1

#. Tap the reset button twice quickly to enter bootloader mode

#. Flash the image:

   .. zephyr-app-commands::
      :zephyr-app: samples/hello_world
      :board: adafruit_itsybitsy_m4_express
      :goals: flash
      :compact:

   You should see "Hello World! adafruit_itsybitsy_m4_express" in your terminal.

Debugging
=========

In addition to the built-in bootloader, the ItsyBitsy can be flashed and
debugged using a SWD probe such as the Segger J-Link.

#. Connect the board to the probe by connecting the :code:`SWCLK`,
   :code:`SWDIO`, :code:`RESET`, :code:`GND`, and :code:`3V3` pins on the
   ItsyBitsy to the :code:`SWCLK`, :code:`SWDIO`, :code:`RESET`, :code:`GND`,
   and :code:`VTref` pins on the `J-Link`_.

#. Flash the image:

   .. zephyr-app-commands::
      :zephyr-app: samples/hello_world
      :board: adafruit_itsybitsy_m4_express
      :goals: flash
      :flash-args: -r openocd
      :compact:

#. Start debugging:

   .. zephyr-app-commands::
      :zephyr-app: samples/hello_world
      :board: adafruit_itsybitsy_m4_express
      :goals: debug
      :compact:

References
**********

.. target-notes::

.. _Adafruit Learning System:
    https://learn.adafruit.com/introducing-adafruit-itsybitsy-m4

.. _pinouts:
    https://learn.adafruit.com/introducing-adafruit-itsybitsy-m4/pinouts

.. _schematic:
    https://learn.adafruit.com/introducing-adafruit-itsybitsy-m4/downloads

.. _J-Link:
    https://www.segger.com/products/debug-probes/j-link/technology/interface-description/
