.. zephyr:board:: stm32u5g9j_dk1

Overview
********

The STM32U5G9J-DK1 Discovery kit is a complete demonstration and development
platform for the STM32U5G9NJH6Q microcontroller, featuring an Arm |reg| Cortex |reg|-M33
core with Arm |reg| TrustZone |reg|.

Leveraging the innovative ultra-low-power oriented features, 3 Mbytes of
embedded SRAM, 4 Mbytes of embedded flash memory, and rich graphics features,
the STM32U5G9J-DK1 Discovery kit enables users to easily prototype applications
with state-of-the-art energy efficiency, as well as providing stunning and
optimized graphics rendering with the support of the 2.5D NeoChrom Accelerator,
Chrom-ART Accelerator, and Chrom-GRC™ MMU.

The full range of hardware features available on the board helps users to enhance
their application development by an evaluation of all the peripherals such as a
2.47-inch RGB 480 x 480 pixels TFT round LCD module with MIPI DSI |reg| interface and
capacitive touch panel, USB Type-C |reg| HS, Octo-SPI flash memory device, Hexadeca-SPI
PSRAM memory device, eMMC flash memory device, Time-of-Flight and gesture detection
sensor, temperature sensor, 20-pin audio MEMS connector, and two 2.54 mm pitch
double-row flexible expansion connectors for easy prototyping with daughterboards
for specific applications (USART, LPUART, two SPIs, SAI, three I2C, SDMMC, ADCs,
timers, and GPIOs).

The STM32U5G9J-DK1 Discovery kits integrate an STLINK-V3E embedded in-circuit
debugger and programmer for the STM32 microcontroller with a USB Virtual COM port
bridge and comes with the STM32CubeU5 MCU Package, which provides an STM32
comprehensive software HAL library as well as various software.

More information about the board can be found at the `STM32U5G9J-DK1 website`_.
More information about STM32U5A9NJH6Q can be found here:

- `STM32U5G9NJ on www.st.com`_
- `STM32U5 Series reference manual`_
- `STM32U5Gxxx datasheet`_

Supported Features
==================

.. zephyr:board-supported-hw::

Pin Mapping
===========

For more details please refer to `STM32U5G9J-DK1 board User Manual`_.

Default Zephyr Peripheral Mapping:
----------------------------------

- USART_1 TX/RX : PA9/PA10 (ST-Link Virtual Port Com)
- LD3 (GREEN) : PE0
- LD4 (RED) : PE1
- User Button: PC13
- USART_3 TX/RX : PB10/PB11
- LPUART_1 TX/RX : PG7/PG8
- I2C1 SCL/SDA : PG14/PG13
- I2C2 SCL/SDA : PF1/PF0
- I2C6 SCL/SDA : PD1/PD0
- SPI2 SCK/MISO/MOSI/CS : PB13/PD3/PD4/PB12
- SPI3 SCK/MISO/MOSI/CS : PG9/PG10/PG11/PG15
- ADC1 : channel5 PA0, channel14 PC5
- ADC2 : channel9 PA4
- ADC4 : channel5 PF14

System Clock
============

The STM32U5G9J-DK1 Discovery kit relies on an HSE oscillator (16 MHz crystal)
and an LSE oscillator (32.768 kHz crystal) as clock references.
Using the HSE (instead of HSI) is mandatory to manage the DSI interface for
the LCD module and the USB high-speed interface.

Serial Port
===========

The STM32U5G9J Discovery kit has up to 4 USARTs, 2 UARTs, and 1 LPUART.
The Zephyr console output is assigned to USART1 is which connected to the onboard
ST-LINK/V3.0. Virtual COM port interface. Default communication settings are
115200 8N1.


Programming and Debugging
*************************

.. zephyr:board-supported-runners::

STM32U5G9J Discovery kit includes an ST-LINK/V3 embedded debug tool interface.
This probe allows to flash and debug the board using various tools.

Flashing
========

The board is configured to be flashed using west `STM32CubeProgrammer`_ runner,
so its :ref:`installation <stm32cubeprog-flash-host-tools>` is required.

Alternatively, OpenOCD can also be used to flash the board using
the ``--runner`` (or ``-r``) option:

.. code-block:: console

   $ west flash --runner openocd

Flashing an application to STM32U5G9J_DK
----------------------------------------

Connect the STM32U5G9J Discovery board to your host computer using the USB
port, then run a serial host program to connect with your Discovery
board. For example:

.. code-block:: console

   $ minicom -D /dev/ttyACM0 -b 115200

Then, build and flash in the usual way. Here is an example for the
:zephyr:code-sample:`hello_world` application.

.. zephyr-app-commands::
   :zephyr-app: samples/hello_world
   :board: stm32u5g9j_dk1
   :goals: build flash

You should see the following message on the console:

.. code-block:: console

   Hello World! stm32u5g9j_dk1

Debugging
=========

Default debugger for this board is OpenOCD. It could be used in the usual way
with "west debug" command.
Here is an example for the :zephyr:code-sample:`blinky` application.

.. zephyr-app-commands::
   :zephyr-app: samples/basic/blinky
   :board: stm32u5g9j_dk1
   :goals: debug


.. _STM32U5G9J-DK1 website:
   https://www.st.com/en/evaluation-tools/stm32u5g9j-dk1.html

.. _STM32U5G9J-DK1 board User Manual:
   https://www.st.com/resource/en/user_manual/um2967-discovery-kits-with-stm32u5x9nj-mcus-stmicroelectronics.pdf

.. _STM32U5G9NJ on www.st.com:
   https://www.st.com/en/microcontrollers-microprocessors/stm32u5g9nj.html

.. _STM32U5 Series reference manual:
   https://www.st.com/resource/en/reference_manual/rm0456-stm32u5-series-armbased-32bit-mcus-stmicroelectronics.pdf

.. _STM32U5Gxxx datasheet:
   https://www.st.com/resource/en/datasheet/stm32u5g9nj.pdf

.. _STM32CubeProgrammer:
   https://www.st.com/en/development-tools/stm32cubeprog.html

.. _STM32U5G9J_DK1 board schematics:
   https://www.st.com/resource/en/schematic_pack/mb1829-u5a9njq-b01-schematic.pdf
