.. zephyr:board:: stm32l496g_disco

Overview
********

The STM32L496G Discovery board features an ARM Cortex-M4 based STM32L496AG MCU
with a wide range of connectivity support and configurations. Here are
some highlights of the STM32L496G Discovery board:


- STM32L496AGI6 microcontroller featuring 1 Mbyte of Flash memory and 320 Kbytes of RAM in an UFBGA169 package
- 1.54 inch 240 x 240 pixel-TFT color LCD with parallel interface
- SAI Audio CODEC, with a stereo headset jack, including analog microphone input
- Stereo digital MEMS microphones
- microSD card connector (card included)
- Camera 8 bit-connector
- 8 Mbit-PSRAM
- IDD measurement
- 64 Mbit-Quad-SPI Flash
- USB OTG FS with Micro-AB connector
- Two types of extension resources:

  - STMod+ and PMOD connectors
  - Compatible Arduino* Uno V3 connectors

- On-board ST-LINK/V2-1 debugger/programmer with SWD connector
- 5 source options for power supply

  - ST-LINK/V2-1 USB connector
  - User USB FS connector
  - VIN from Arduino connector
  - 5 V from Arduino connector
  - USB charger
  - USB VBUS or external source(3.3V, 5V, 7 - 12V)
  - Power management access point

- 8 LEDs
- Reset push button
- 4 direction-joystick with selection

More information about the board can be found at the `STM32L496G Discovery website`_.

Hardware
********

The STM32L496AG SoC provides the following hardware capabilities:

- Ultra-low-power with FlexPowerControl (down to 108 nA Standby mode and 91
  |micro| A/MHz run mode)
- Core: ARM |reg| 32-bit Cortex |reg| -M4 CPU with FPU, frequency up to 80 MHz,
  100DMIPS/1.25DMIPS/MHz (Dhrystone 2.1)
- Clock Sources:

  - 4 to 48 MHz crystal oscillator
  - 32 kHz crystal oscillator for RTC (LSE)
  - Internal 16 MHz factory-trimmed RC ( |plusminus| 1%)
  - Internal low-power 32 kHz RC ( |plusminus| 5%)
  - Internal multispeed 100 kHz to 48 MHz oscillator, auto-trimmed by
    LSE (better than |plusminus| 0.25 % accuracy)
  - Internal 48 MHz with clock recovery
  - 3 PLLs for system clock, USB, audio, ADC

- RTC with HW calendar, alarms and calibration
- LCD 8 x 40 or 4 x 44 with step-up converter
- Up to 24 capacitive sensing channels: support touchkey, linear and rotary touch sensors
- 16x timers:

  - 2x 16-bit advanced motor-control
  - 2x 32-bit and 5x 16-bit general purpose
  - 2x 16-bit basic
  - 2x low-power 16-bit timers (available in Stop mode)
  - 2x watchdogs
  - SysTick timer

- Up to 136 fast I/Os, most 5 V-tolerant, up to 14 I/Os with independent supply down to 1.08 V
- Memories

  - Up to 1 MB Flash, 2 banks read-while-write, proprietary code readout protection
  - 320 KB of SRAM including 64 KB with hardware parity check
  - External memory interface for static memories supporting SRAM, PSRAM, NOR, and NAND memories
  - Quad SPI memory interface

- 4x digital filters for sigma delta modulator
- Rich analog peripherals (independent supply)

  - 3x 12-bit ADC 5 MSPS, up to 16-bit with hardware oversampling, 200
    |micro| A/MSPS
  - 2x 12-bit DAC, low-power sample and hold
  - 2x operational amplifiers with built-in PGA
  - 2x ultra-low-power comparators

- 20x communication interfaces

  - USB OTG 2.0 full-speed, LPM and BCD
  - 2x SAIs (serial audio interface)
  - 4x I2C FM+(1 Mbit/s), SMBus/PMBus
  - 5x USARTs (ISO 7816, LIN, IrDA, modem)
  - 1x LPUART
  - 3x SPIs (4x SPIs with the Quad SPI)
  - 2x CAN (2.0B Active) and SDMMC interface
  - SWPMI single wire protocol master I/F
  - IRTIM (Infrared interface)

- 14-channel DMA controller
- True random number generator
- CRC calculation unit, 96-bit unique ID
- Development support: serial wire debug (SWD), JTAG, Embedded Trace Macrocell*


More information about STM32L496AG can be found in:

- `STM32L496AG on www.st.com`_
- `STM32L496 reference manual`_

Supported Features
==================

.. zephyr:board-supported-hw::

Connections and IOs
===================

STM32L496G Discovery Board has 8 GPIO controllers. These controllers are responsible for pin muxing,
input/output, pull-up, etc.

For more details please refer to `STM32L496G Discovery board User Manual`_.

Default Zephyr Peripheral Mapping:
----------------------------------

- UART_1 TX/RX : PB6/PG10
- UART_2 TX/RX : PA2/PD6 (ST-Link Virtual Port Com)
- LPUART_1 TX/RX : PG7/PG8 (Arduino Serial)
- I2C1 SCL/SDA : PB8/PB7 (Arduino I2C)
- SDMMC_1 D0/D1/D2/D3/CK/CMD: PC8/PC9/PC10/PC11/PC12/PD2
- SPI1 NSS/SCK/MISO/MOSI : PA15/PA5/PB4/PB5 (Arduino SPI)
- USB DM/DP/ID : PA11/PA12/PA10
- I2C_1_SCL : PB8
- I2C_1_SDA : PB7
- PWM_2_CH1 : PA0
- LD2 : PB13

System Clock
------------

STM32L496G Discovery System Clock could be driven by an internal or external oscillator,
as well as the main PLL clock. By default the System clock is driven by the PLL clock at 80MHz,
driven by 16MHz high speed internal oscillator.

Serial Port
-----------

STM32L496G Discovery board has 5 U(S)ARTs. The Zephyr console output is assigned to UART2.
Default settings are 115200 8N1.


Programming and Debugging
*************************

.. zephyr:board-supported-runners::

STM32L496G Discovery board includes an ST-LINK/V2-1 embedded debug tool interface.

Flashing
========

The board is configured to be flashed using west `STM32CubeProgrammer`_ runner,
so its :ref:`installation <stm32cubeprog-flash-host-tools>` is required.

Alternatively, OpenOCD or JLink can also be used to flash the board using
the ``--runner`` (or ``-r``) option:

.. code-block:: console

   $ west flash --runner openocd
   $ west flash --runner jlink

Applications for the ``stm32l496g_disco`` board configuration can be
built and flashed in the usual way (see :ref:`build_an_application`
and :ref:`application_run` for more details).

Flashing an application to STM32L496G Discovery
-----------------------------------------------

Connect the STM32L496G Discovery to your host computer using the USB
port, then run a serial host program to connect with your Discovery
board. For example:

.. code-block:: console

   $ minicom -D /dev/ttyACM0

Then, build and flash in the usual way. Here is an example for the
:zephyr:code-sample:`hello_world` application.

.. zephyr-app-commands::
   :zephyr-app: samples/hello_world
   :board: stm32l496g_disco
   :goals: build flash

You should see the following message on the console:

.. code-block:: console

   Hello World! arm

Debugging
=========

You can debug an application in the usual way.  Here is an example for the
:zephyr:code-sample:`hello_world` application.

.. zephyr-app-commands::
   :zephyr-app: samples/hello_world
   :board: stm32l496g_disco
   :maybe-skip-config:
   :goals: debug

.. _STM32L496G Discovery website:
   https://www.st.com/en/evaluation-tools/32l496gdiscovery.html

.. _STM32L496G Discovery board User Manual:
   https://www.st.com/resource/en/user_manual/dm00353127.pdf

.. _STM32L496AG on www.st.com:
   https://www.st.com/en/microcontrollers/stm32l496ag.html

.. _STM32L496 reference manual:
   https://www.st.com/resource/en/reference_manual/DM00083560.pdf

.. _STM32CubeProgrammer:
   https://www.st.com/en/development-tools/stm32cubeprog.html
