.. _eval_adxl362_ardz:

EVAL-ADXL362-ARDZ
#################

Overview
********

The EVAL-ADXL362-ARDZ is a 3-axis digital accelerometer Arduino shield powered
by the Analog Devices ADXL362.

.. figure:: eval_adxl362_ardz.webp
   :align: center
   :alt: EVAL-ADXL362-ARDZ

Programming
***********

Set ``--shield eval_adxl362_ardz`` when you invoke ``west build``. For example:

.. zephyr-app-commands::
   :zephyr-app: samples/sensor/sensor_shell
   :board: apard32690/max32690/m4
   :shield: eval_adxl362_ardz
   :goals: build

Requirements
************

This shield can only be used with a board which provides a configuration for
Arduino connectors and defines node aliases for SPI and GPIO interfaces (see
:ref:`shields` for more details).

References
**********

- `EVAL-ADXL362-ARDZ product page`_
- `EVAL-ADXL362-ARDZ user guide`_
- `EVAL-ADXL362-ARDZ schematic`_
- `ADXL362 product page`_
- `ADXL362 data sheet`_

.. _EVAL-ADXL362-ARDZ product page:
   https://www.analog.com/en/resources/evaluation-hardware-and-software/evaluation-boards-kits/eval-adxl362-ardz.html

.. _EVAL-ADXL362-ARDZ user guide:
   https://wiki.analog.com/resources/eval/user-guides/eval-adicup360/hardware/adxl362

.. _EVAL-ADXL362-ARDZ schematic:
   https://www.analog.com/media/en/reference-design-documentation/design-integration-files/eval-adxl362-ardz-designsupport.zip

.. _ADXL362 product page:
   https://www.analog.com/en/products/adxl362.html

.. _ADXL362 data sheet:
   https://www.analog.com/media/en/technical-documentation/data-sheets/adxl362.pdf
