.. _x-nucleo-wb05kn1:

X-NUCLEO-WB05KN1: BLE expansion board
#####################################

Overview
********
The X-NUCLEO-WB05KN1 is a Bluetooth Low Energy evaluation board which allows the
expansion of the STM32 Nucleo boards.
The RF module is FCC (FCC ID: YCP-MB203202) and IC certified (IC: 8976A-MB203202).

The X-NUCLEO-WB05KN1 is compatible out of the box with the Arduino UNO R3 connector.
The board interfaces with the host microcontroller via UART (default) or SPI peripheral.
However, the out-of-the-box firmware is not compatible with Zephyr; therefore, a controller-only
image should be flashed on the board using CN8 pin headers.
For more information about how to change the firmware, please refer to `UM3406`_ section 3.3.

.. note::
   The `X-CUBE-WB05N`_ package provided by ST contains firmware compatible with Zephyr
   in the ``Utilities/BLE_Transparent_Mode_STM32WB05_controller_only`` directory
   (``SPI`` or ``UART`` subdirectories depending on which interface you want to use).

.. image:: img/x-nucleo-wb05kn1.webp
     :align: center
     :alt: X-NUCLEO-WB05KN1

More information about the board can be found at the
`X-NUCLEO-WB05KN1 website`_.

Configurations
**************

X-NUCLEO-WB05KN1 can be utilized as a Bluetooth Low-Energy controller shield
with a UART or SPI host controller interface (HCI-UART/HCI-SPI).

The UART default settings are:

* Baudrate: 921600 bps
* 8 bits, no parity, 1 stop bit

+----------+-----------------------+
| UART Pin | Arduino Connector Pin |
+==========+=======================+
| RX       | D0                    |
+----------+-----------------------+
| TX       | D1                    |
+----------+-----------------------+

The SPI default settings are:

* Mode: Full-duplex slave
* Frame format: Motorola
* Data size: 8 bits, MSB first
* Clock Polarity: High (CPOL=1)
* Clock Phase: 2 Edge (CPHA=1)
* CS type: Software-controlled

IRQ and reset pins are also necessary in addition to SPI pins.

+----------------+-----------------------+
| SPI Config Pin | Arduino Connector Pin |
+================+=======================+
| SCK            | D13                   |
+----------------+-----------------------+
| MISO           | D12                   |
+----------------+-----------------------+
| MOSI           | D11                   |
+----------------+-----------------------+
| CS             | D10                   |
+----------------+-----------------------+
| IRQ            | A0                    |
+----------------+-----------------------+
| RESET          | D7                    |
+----------------+-----------------------+

More information about X-NUCLEO-WB05KN1 can be found here:

- `X-NUCLEO-WB05KN1 datasheet`_

Programming
***********

Activate the presence of the shield for the project build by adding the
``--shield x_nucleo_wb05kn1_uart`` or ``--shield x_nucleo_wb05kn1_spi`` when you invoke
``west build`` based on UART or SPI interface:

 .. zephyr-app-commands::
    :app: your_app
    :board: your_board_name
    :shield: x_nucleo_wb05kn1_uart
    :goals: build

Or

 .. zephyr-app-commands::
    :app: your_app
    :board: your_board_name
    :shield: x_nucleo_wb05kn1_spi
    :goals: build

References
**********

.. target-notes::

.. _UM3406:
   https://www.st.com/resource/en/user_manual/um3406-getting-started-with-the-xcubewb05n-bluetooth-low-energy-software-expansion-for-stm32cube-stmicroelectronics.pdf

.. _X-CUBE-WB05N:
   https://www.st.com/en/embedded-software/x-cube-wb05n.html

.. _X-NUCLEO-WB05KN1 website:
   https://www.st.com/en/evaluation-tools/x-nucleo-wb05kn1.html

.. _X-NUCLEO-WB05KN1 datasheet:
   https://www.st.com/resource/en/datasheet/stm32wb05kn.pdf
