.. zephyr:board:: raytac_mdbt53v_db_40

Overview
********

Raytac MDBT53V-DB-40 demo board is a development board based on the Raytac MDBT53V-1M module,
using Nordic Semiconductor nRF5340 ARM Cortex-M33 SoC. Its design concept is to connect all
of the module's pins to 2.54mm pin headers. It is convenient for developers to verify whether
the modules are connected to other peripheral devices or sensors as a tool for software development.

The nRF5340 inside the MDBT53V-1M module is a
dual-core SoC based on the Arm® Cortex®-M33 architecture, with:

* a full-featured Arm Cortex-M33F core with DSP instructions, FPU, and
  Armv8-M Security Extension, running at up to 128 MHz, referred to as
  the **application core**
* a secondary Arm Cortex-M33 core, with a reduced feature set, running
  at a fixed 64 MHz, referred to as the **network core**.

The raytac_mdbt53v_db_40_nrf5340_cpuapp build target provides support for the application
core on the nRF5340 SoC. The raytac_mdbt53v_db_40_nrf5340_cpuapp build target provides
support for the network core on the nRF5340 SoC.

nRF5340 SoC provides support for the following devices:

* :abbr:`ADC (Analog to Digital Converter)`
* CLOCK
* FLASH
* :abbr:`GPIO (General Purpose Input Output)`
* :abbr:`IDAU (Implementation Defined Attribution Unit)`
* :abbr:`I2C (Inter-Integrated Circuit)`
* :abbr:`MPU (Memory Protection Unit)`
* :abbr:`NVIC (Nested Vectored Interrupt Controller)`
* :abbr:`PWM (Pulse Width Modulation)`
* RADIO (Bluetooth Low Energy and 802.15.4)
* :abbr:`RTC (nRF RTC System Clock)`
* Segger RTT (RTT Console)
* :abbr:`SPI (Serial Peripheral Interface)`
* :abbr:`UARTE (Universal asynchronous receiver-transmitter)`
* :abbr:`WDT (Watchdog Timer)`

More information about the board can be found at the `MDBT53V-DB-40 website`_.
The `MDBT53V-DB-40 Specification`_ contains the demo board's datasheet.
The `MDBT53V-DB-40 Schematic`_ contains the demo board's schematic.

Hardware
********
- Module Demo Board build by MDBT53V-1M
- Nordic nRF5340 SoC Solution
- A recommended 3rd-party module by Nordic Semiconductor.
- Dual-core Arm® Cortex®-M33
- 1MB/256KB Flash Memory; 512kB/ 64kB RAM
- Supports BT5 Long Range Features
- Bluetooth specification v5.2
- Supports BT5 Long Range Features
- Supports Bluetooth Direction Finding & Mesh
- Supports Bluetooth low energy audio
- Certifications: FCC, IC, CE, Telec(MIC), KC, SRRC, NCC, RCM, WPC
- RoHs & Reach Compliant.
- 25 GPIO
- Chip Antenna
- Interfaces: SPI, UART, I2C, I2S, PWM, ADC, and NFC
- Highly flexible multiprotocol SoC ideally suited for Bluetooth® Low Energy, ANT+, Zigbee, Thread (802.15.4) ultra low-power wireless applications.
- 1 User LEDs
- 3 User buttons
- 1 Mini USB connector for power supply
- SWD connector for FW programming
- J-Link interface for FW programming

Supported Features
==================

.. zephyr:board-supported-hw::

See `MDBT53V-DB-40 website`_ and `MDBT53V-DB-40 Specification`_
for a complete list of Raytac MDBT53V-DB-40 board hardware features.

Connections and IOs
===================

LED
---

* LED1 (green) = P0.31

Push buttons
------------

* BUTTON1 = SW1 = P1.13
* BUTTON2 = SW2 = P0.25
* BUTTON3 = SW3 = P0.26

HSPI
----
* MOSI = P0.9
* MISO = P0.10
* SCK = P0.8
* CSN = P0.11
* DCX = P0.12

QSPI
----
* SCK = P0.17
* CSN = P0.18
* DATA0 = P0.13
* DATA1 = P0.14
* DATA2 = P0.15
* DATA3 = P0.16

Security components
===================

- Implementation Defined Attribution Unit (`IDAU`_) on the application core.
  The IDAU is implemented with the System Protection Unit and is used to
  define secure and non-secure memory maps.  By default, all of the memory
  space  (Flash, SRAM, and peripheral address space) is defined to be secure
  accessible only.
- Secure boot.

Programming and Debugging
*************************

.. zephyr:board-supported-runners::

nRF5340 application core supports the Armv8-M Security Extension.
Applications built for the raytac_mdbt53v_db_40_nrf5340_cpuapp board by
default boot in the Secure state.

nRF5340 network core does not support the Armv8-M Security Extension.
nRF5340 IDAU may configure bus accesses by the nRF5340 network core
to have Secure attribute set; the latter allows to build and run
Secure only applications on the nRF5340 SoC.

Applications for the ``raytac_mdbt53v_db_40_nrf5340`` board configuration can be
built, flashed, and debugged in the usual way. See :ref:`build_an_application` and
:ref:`application_run` for more details on building and running.

.. note::
   Flashing and Debugging Zephyr onto the raytac_mdbt53v_db_40_nrf5340 board
   requires an	external J-Link programmer. The programmer is attached to the J1
   or J9 SWD connector.


Flashing
========

Follow the instructions in the :ref:`nordic_segger` page to install
and configure all the necessary software. Further information can be
found in :ref:`nordic_segger_flashing`. Then build and flash
applications as usual (see :ref:`build_an_application` and
:ref:`application_run` for more details).

Here is an example for the :zephyr:code-sample:`hello_world` application.

Use a USB to TTL converter to connect the computer and raytac_mdbt53v_db_40_nrf5340
J13 connector pin 8(RX), 9(TX) and GND. Then run your favorite terminal program to listen for output.

.. code-block:: console

   $ minicom -D <tty_device> -b 115200

Replace :code:`<tty_device>` with the port where the USB to TTL converter
can be found. For example, under Linux, :code:`/dev/ttyUSB0`.

Then build and flash the application in the usual way.

.. zephyr-app-commands::
   :zephyr-app: samples/hello_world
   :board: raytac_mdbt53v_db_40_nrf5340
   :goals: build flash

Debugging
=========

The ``raytac_mdbt53v_db_40_nrf5340`` board does not have an on-board-J-Link debug IC,
however, instructions from the :ref:`nordic_segger` page also apply to this board.
Use the Debug out connector of nRF52x DK to connect to the J1 connector, and use SEGGER
J-Link OB IF to debug.


References
**********

.. target-notes::

.. _IDAU:
   https://developer.arm.com/docs/100690/latest/attribution-units-sau-and-idau
.. _MDBT53V-DB-40 website:
	https://www.raytac.com/product/ins.php?index_id=140
.. _MDBT53V-DB-40 Specification:
	https://www.raytac.com/download/index.php?index_id=62
.. _MDBT53V-DB-40 Schematic:
	https://www.raytac.com/upload/catalog_b/f2c33d52dca8cd6546c95938bc0cb295.jpg
.. _J-Link Software and documentation pack:
	https://www.segger.com/jlink-software.html
