.. zephyr:board:: esp32c3_lckfb

Overview
********

The LCKFB ESP32-C3 is a feature-rich development board built around the ESP32-C3 SoC with 8 MB of onboard SPI flash. It offers full Wi-Fi and Bluetooth Low Energy connectivity, complemented by a comprehensive set of sensors, audio capabilities, and display interfaces.

The board is designed for IoT applications requiring motion sensing, environmental monitoring,
audio processing, and graphical display capabilities.

For more information, check `LCKFB ESP32-C3 Development Board`_.

Hardware
********

.. include:: ../../../espressif/common/soc-esp32c3-features.rst
   :start-after: espressif-soc-esp32c3-features

Supported Features
==================

.. zephyr:board-supported-hw::

System Requirements
*******************

.. include:: ../../../espressif/common/system-requirements.rst
   :start-after: espressif-system-requirements

Programming and Debugging
*************************

.. zephyr:board-supported-runners::

.. include:: ../../../espressif/common/building-flashing.rst
   :start-after: espressif-building-flashing

.. include:: ../../../espressif/common/board-variants.rst
   :start-after: espressif-board-variants

Debugging
=========

.. include:: ../../../espressif/common/openocd-debugging.rst
   :start-after: espressif-openocd-debugging

References
**********

.. target-notes::

.. _`LCKFB ESP32-C3 Development Board`: https://wiki.lckfb.com/zh-hans/szpi-esp32c3/
