# mqseries_cmit

(PECL mqseries >= 0.10.0)

mqseries_cmit — MQSeries MQCMIT

### 说明

mqseries_cmit ( resource `$hconn` , resource `&$compCode` , resource `&$reason` ) : void

The mqseries_cmit() (MQCMIT) call indicates to the queue manager that the application has reached a syncpoint, and that all of the message gets and puts that have occurred since the last syncpoint are to be made permanent. Messages put as part of a unit of work are made available to other applications; messages retrieved as part of a unit of work are deleted.

### 参数

`hConn`

  Connection handle.

  This handle represents the connection to the queue manager.

`compCode`

  Completion code.

`reason`

  Reason code qualifying the compCode.

### 返回值

没有返回值。

### 范例

Example #1 mqseries_cmit() example

    <?php
        mqseries_cmit($conn, $comp_code, $reason);
        if ($comp_code !== MQSERIES_MQCC_OK) {
            printf("cmit CompCode:%d Reason:%d Text:%s<br>\n", $comp_code, $reason, mqseries_strerror($reason));
        }
    ?>

### 注释

> Note:

> mqseries_back() will not function when using MQSeries Client to connect to a Queueu Manager.

### 参见

- mqseries_begin() - MQseries MQBEGIN
- mqseries_back() - MQSeries MQBACK
- mqseries_conn() - MQSeries MQCONN
- mqseries_connx() - MQSeries MQCONNX