- dm gpio driver
- ethernet driver for the dm9000
- reduce the hundreds of definitions of register addresses to the ones really needed in assembly or SPL.
- define the remaining register base addresses as physical addresses and establish a mapping with ioremap_nocache()
