* Freescale ColdFire FEC ethernet controller

Required properties:
- compatible: should be "fsl,mcf-fec"
- reg: address and length of the register set for the device.

Optional properties:
- mii-base: index of FEC reg area, 0 for FEC0, 1 for FEC1
- max-speed: max speedm Mbits/sec
- phy-addr: phy address
- timeout-loop: integer value for driver loops time out


Example:

fec0: ethernet@fc030000 {
	compatible = "fsl,mcf-fec";
	reg = <0xfc030000 0x400>;
	mii-base = <0>;
	phy-addr = <0>;
	timeout-loop = <5000>;
};
