U-Boot bootcounter Devicetree Binding
=====================================

The device tree node describes the U-Boot bootcounter
memory based device binding.

Required properties :

- compatible : "u-boot,bootcount";
- single-word : set this, if you have only one word space
    for storing the bootcounter.

Example
-------

MPC83xx based board:

bootcount@0x13ff8 {
	compatible = "u-boot,bootcount";
	reg = <0x13ff8 0x08>;
};
