Axis Communications AB
ARTPEC series SoC Device Tree Bindings

ARTPEC-6 ARM SoC
================

Required root node properties:
- compatible = "axis,artpec6";

ARTPEC-6 Development board:
---------------------------
Required root node properties:
- compatible = "axis,artpec6-dev-board", "axis,artpec6";
