* broadcom bcm6838 pinctrl

Required properties for the pinctrl driver:
- compatible:	   "brcm,bcm6838-pinctrl"
- regmap:		   specify the gpio test port syscon
- brcm,pins-count:      the number of pin
- brcm,functions-count: the number of function

Please refer to pinctrl-bindings.txt in this directory for details of the
common pinctrl bindings used by client devices.

Example:

		gpio_test_port: syscon@14e00294 {
			compatible = "syscon";
			reg = <0x14e00294 0x1c>;
		};

		pinctrl: pinctrl {
			compatible = "brcm,bcm6838-pinctrl";
			regmap = <&gpio_test_port>;
			brcm,pins-count = <74>;
			brcm,functions-count = <8>;

			usb0: usb0 {
				usb0_pwrflt {
					pins = "69";
					function = "1";
				};
				usb0_pwron {
					pins = "70";
					function = "1";
				};
			};
		};
