Main Page Class List Class Members

# Nv Namespace Reference

## Namespaces
namespace | Blast

## Detailed Description

FractureTool has requirements to input meshes to fracture them successfully: 1) Mesh should be closed (watertight) 2) There should not be self-intersections and open-edges. Mesh cleaner input is closed mesh with self-intersections and open-edges (only in the interior). It tries to track outer hull to make input mesh solid and meet requierements of FractureTool. If mesh contained some internal cavities they will be removed.

Blast serialization support for the ExtPhysX extension. Contains serializers which can be used by the ExtSerialization manager.

Blast High-level serialization support. Contains serializers which can be used by the ExtSerialization manager.

This file contains AllocatorCallback wrappers compatible with PxShared containers.