This parameter determines how far away a slope can be to affect the spreading of this fluid. Instead of spreading evenly, 
the fluid will try to reach the slope. With lower values, the fluid will usually cover larger areas if the ground is uneven.