Snort does a lot of work and outputs some useful statistics when it is done.
Many of these are self-explanatory.  The others are summarized below.  This
does not include all possible output data, just the basics.


-----------------
Timing Statistics
-----------------

This section provides basic timing statistics.  It includes total seconds and
packets as well as packet processing rates.  The rates are based on whole
seconds, minutes, etc. and only shown when non-zero.

Example:

===============================================================================
Run time for packet processing was 175.856509 seconds
Snort processed 3716022 packets.
Snort ran for 0 days 0 hours 2 minutes 55 seconds
   Pkts/min:      1858011
   Pkts/sec:        21234
===============================================================================


-----------------
Packet I/O Totals
-----------------

This section shows basic packet acquisition and injection peg counts obtained
from the DAQ.  If you are reading pcaps, the totals are for all pcaps combined,
unless you use --pcap-reset, in which case it is shown per pcap.

* Outstanding indicates how many packets are buffered awaiting processing.  The
  way this is counted varies per DAQ so the DAQ documentation should be
  consulted for more info.

* Filtered packets are not shown for pcap DAQs.

* Injected packets are the result of active response which can be configured for
  inline or passive modes.

Example:

===============================================================================
Packet I/O Totals:
   Received:      3716022
   Analyzed:      3716022 (100.000%)
    Dropped:            0 (  0.000%)
   Filtered:            0 (  0.000%)
Outstanding:            0 (  0.000%)
   Injected:            0
===============================================================================


-------------------
Protocol Statistics
-------------------

Traffic for all the protocols decoded by Snort is summarized in the breakdown
section.  This traffic includes internal "pseudo-packets" if preprocessors such
as frag3 and stream5 are enabled so the total may be greater than the number of
analyzed packets in the packet I/O section.

* Disc counts are discards due to basic encoding integrity flaws that prevents
  Snort from decoding the packet.

* Other includes packets that contained an encapsulation that Snort doesn't
  decode.

* S5 G 1/2 is the number of client/server sessions stream5 flushed due to cache
  limit, session timeout, session reset.

Example:

===============================================================================
Breakdown by protocol (includes rebuilt packets):
        Eth:      3722347 (100.000%)
       VLAN:            0 (  0.000%)
        IP4:      1782394 ( 47.884%)
       Frag:         3839 (  0.103%)
       ICMP:        38860 (  1.044%)
        UDP:       137162 (  3.685%)
        TCP:      1619621 ( 43.511%)
        IP6:      1781159 ( 47.850%)
    IP6 Ext:      1787327 ( 48.016%)
   IP6 Opts:         6168 (  0.166%)
      Frag6:         3839 (  0.103%)
      ICMP6:         1650 (  0.044%)
       UDP6:       140446 (  3.773%)
       TCP6:      1619633 ( 43.511%)
     Teredo:           18 (  0.000%)
    ICMP-IP:            0 (  0.000%)
      EAPOL:            0 (  0.000%)
    IP4/IP4:            0 (  0.000%)
    IP4/IP6:            0 (  0.000%)
    IP6/IP4:            0 (  0.000%)
    IP6/IP6:            0 (  0.000%)
        GRE:          202 (  0.005%)
    GRE Eth:            0 (  0.000%)
   GRE VLAN:            0 (  0.000%)
    GRE IP4:            0 (  0.000%)
    GRE IP6:            0 (  0.000%)
GRE IP6 Ext:            0 (  0.000%)
   GRE PPTP:          202 (  0.005%)
    GRE ARP:            0 (  0.000%)
    GRE IPX:            0 (  0.000%)
   GRE Loop:            0 (  0.000%)
       MPLS:            0 (  0.000%)
        ARP:       104840 (  2.817%)
        IPX:           60 (  0.002%)
   Eth Loop:            0 (  0.000%)
   Eth Disc:            0 (  0.000%)
   IP4 Disc:            0 (  0.000%)
   IP6 Disc:            0 (  0.000%)
   TCP Disc:            0 (  0.000%)
   UDP Disc:         1385 (  0.037%)
  ICMP Disc:            0 (  0.000%)
All Discard:         1385 (  0.037%)
      Other:        57876 (  1.555%)
Bad Chk Sum:        32135 (  0.863%)
    Bad TTL:            0 (  0.000%)
     S5 G 1:         1494 (  0.040%)
     S5 G 2:         1654 (  0.044%)
      Total:      3722347
===============================================================================


-----------------------------
Actions, Limits, and Verdicts
-----------------------------

Action and verdict counts show what Snort did with the packets it analyzed.
This information is only output in IDS mode (when snort is run with the -c
<conf> option).

* Alerts is the number of activate, alert, and block actions processed as
  determined by the rule actions.  Here block includes block, drop, and reject
  actions.

Limits arise due to real world constraints on processing time and available
memory.  These indicate potential actions that did not happen:

* Match Limit > 0 means that rule matches were not processed due to the 
  config detection: max_queue_events setting.  The default is 5.

* Queue Limit > 0 means that events couldn't be stored in the event queue
  due to the config event_queue: max_queue setting.  The default is 8.

* Log Limit > 0 means that events were not alerted due to the 
  config event_queue: log setting.  The default is 3.

* Event Limit > 0 means that events were not alerted due to event_filter
  limits.

* Alert Limit > 0 means that events were not alerted because they already
  were triggered on the session.

Verdicts are rendered by Snort on each packet:

* Allow = packets Snort analyzed and did not take action on. 

* Block = packets Snort did not forward, e.g. due to a block rule.  "Block" is
  used instead of "Drop" to avoid confusion between dropped packets (those
  Snort didn't actually see) and blocked packets (those Snort did not allow to
  pass).

* Replace = packets Snort modified, for example, due to normalization or
  replace rules.  This can only happen in inline mode with a compatible DAQ.

* Whitelist = packets that caused Snort to allow a flow to pass w/o inspection
  by any analysis program.  Like blacklist, this is done by the DAQ or by Snort
  on subsequent packets.

* Blacklist = packets that caused Snort to block a flow from passing.  This is
  the case when a block TCP rule fires.  If the DAQ supports this in hardware,
  no further packets will be seen by Snort for that session.  If not, snort
  will block each packet and this count will be higher.

* Ignore = packets that caused Snort to allow a flow to pass w/o inspection
  by this instance of Snort.  Like blacklist, this is done by the DAQ or by
  Snort on subsequent packets.

* Int Blklst = packets that are GTP, Teredo, 6in4 or 4in6 encapsulated that
  are being blocked.  These packets could get the Blacklist verdict if 
  config tunnel_verdicts was set for the given protocol.  Note that these 
  counts are output only if non-zero.  Also, this count is incremented on 
  the first packet in the flow that alerts.  The alerting packet and all
  following packets on the flow will be counted under Block.

* Int Whtlst = packets that are GTP, Teredo, 6in4 or 4in6 encapsulated that
  are being allowed.  These packets could get the Whitelist verdict if 
  config tunnel_verdicts was set for the given protocol.  Note that these
  counts are output only if non-zero.  Also, this count is incremented
  for all packets on the flow starting with the alerting packet.

Example:

===============================================================================
Action Stats:
     Alerts:            0 (  0.000%)
     Logged:            0 (  0.000%)
     Passed:            0 (  0.000%)
Limits:
      Match:            0
      Queue:            0
        Log:            0
      Event:            0
      Alert:            0
Verdicts:
      Allow:      3716022 (100.000%)
      Block:            0 (  0.000%)
    Replace:            0 (  0.000%)
  Whitelist:            0 (  0.000%)
  Blacklist:            0 (  0.000%)
     Ignore:            0 (  0.000%)
===============================================================================

