# SSEC 89 GHz AMSU-B Brightness Temperature (BT)

THis enhancement is a reproduction of the SSEC 89 GHz brightness temperature color scale originally intended for AMSU-B, then applied to MHS and AMSU-A.

### Appearance

The temperature range displayed starts at -94°C and ends at 4°C.

### Intended usage

Cyclone/hurricane convection monitoring

### Limitations

No specific limitations.

### References

[SSEC](https://tropic.ssec.wisc.edu/real-time/amsu/explanation.html)
