# 10.8 µm Thermal IR (uncalibrated)

Selects the thermal infrared (10.8 µm) channel and equalizes it.

This enhancement is NOT calibrated in temperature.

### Appearance

Colder temperatures appear white while warmer temperatures appear progressively darker shades of black.

### Intended usage

Qualitative temperature analysis

### Limitations

No emissivity compensation.
No calibration (qualitiative analysis only).