# Panchromatic

The panchromatic band on VIIRS-DNB uses a single band that combines red, green, and blue bands.
The resulting image does not contain any wavelength-specific information.

### Appearance

Grayscale

### Intended usage

Pansharpening of lower resolution channels.

### Limitations

* Sensitive Rayleigh scattering.
* Sensitive to atmospheric haze.