Project Settings
Project Name | synplify_pro | Device Name | synplify_impl: Pango Logos : PGL22G
Implementation Name | synplify_impl | Top Module | ipsl_hmemc_top_test
Pipelining | 1 | Retiming | 0
Resource Sharing | 1 | Fanout Guide | 10000
Disable I/O Insertion | 0 | Disable Sequential Optimizations | 0
Clock Conversion | 1 | FSM Compiler | 1
Run Status
Job Name | Status |  |  |  | CPU Time | Real Time | Memory | Date/Time
(compiler) | Complete | 97 | 494 | 0 | - | 00m:01s | - | 2019/5/7 16:40:49
(premap) | Complete | 22 | 91 | 0 | 0m:03s | 0m:03s | 232MB | 2019/5/7 16:40:53
(fpga_mapper) | Complete | 429 | 452 | 0 | 0m:34s | 0m:44s | 460MB | 2019/5/7 16:41:38
Area Summary
I/O ports (io_port) | 78 | Dedicated Rams (v_ram) | 4 (48)
Distributed Rams | 30.00 (1110) | LUTs (total_luts) | 2079 (11%)
Timing Summary
Clock Name | Req Freq | Est Freq | Slack
--- | --- | --- | ---
ipsl_ddrphy_dll_update_ctrl|dll_update_n_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|IOCLK_DIV_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[2] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[3] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[4] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[5] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[6] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[7] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[9] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[10] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[11] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[12] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[17] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[18] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[19] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[20] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[21] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[22] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[23] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[24] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[25] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[27] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[28] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[29] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[31] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[32] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[33] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[34] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[35] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[36] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[37] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[40] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[41] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[42] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[43] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[44] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[45] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[46] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[47] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[48] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[49] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[51] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[52] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[55] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[56] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[57] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[58] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_clk_sys_inferred_clock[59] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_dqs_clk_regional_inferred_clock[0] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_dqs_clk_regional_inferred_clock[1] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_dqs_clk_regional_inferred_clock[2] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_dqs_clk_regional_inferred_clock[3] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|buffer_dqs_clk_regional_inferred_clock[4] | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs0_clk_r_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs1_clk_r_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs_90_0_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs_90_1_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs_ca_clk_r_01_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs_ca_clk_r_03_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs_ca_clk_r_04_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs_clkw290_0_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs_clkw290_1_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs_clkw_0_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs_clkw_1_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs_clkw_ca_01_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs_clkw_ca_03_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|dqs_clkw_ca_04_inferred_clock | 1.0 MHz | NA | NA
ipsl_phy_io_Z8|ioclk_01_inferred_clock | 1.0 MHz | 1008.1 MHz | 999.008
ipsl_phy_io_Z8|ioclk_02_inferred_clock | 1.0 MHz | NA | NA
pll_50_400|clkout1_inferred_clock | 1.0 MHz | 120.6 MHz | 991.706
pll_50_400|clkout3_inferred_clock | 1.0 MHz | 150.7 MHz | 993.364
sys_clk | 50.0 MHz | 197.4 MHz | 14.934
video_pll|clkout0_inferred_clock | 1.0 MHz | 179.2 MHz | 994.419
video_pll|clkout1_inferred_clock | 1.0 MHz | 734.4 MHz | 998.638
System | 1.0 MHz | 780.5 MHz | 998.719
Optimizations Summary
Combined Clock Conversion | 1 / 75 |  |