# ac001

This is an enter key with rgb .

* Keyboard Maintainer: [jonylee@hfd](https://github.com/jonylee1986)
* Hardware Supported: ac001

Make example for this keyboard (after setting up your build environment):

    make hfdkb/ac001:default

Flashing example for this keyboard:

    make hfdkb/ac001:default:flash


See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

Enter the bootloader:

* **Bootmagic reset**: Hold down the encoder and plug in the keyboard
* **Physical reset button**: Briefly press the button on the back of the PCB
