# Default Genesis Macro Pad Layout

This is the default layout for the Genesis Macro Pad. It assumes all 1u switches 
and optional rotary encoder in the top-left or top-right corner for media volume 
control. The top left switch activates Layer 1 which enables control of the RGB
underglow.