# Resume1800

![Resume1800](https://i.imgur.com/IjP3Opwh.jpg)

An 1800 compact keyboard that is built with soley through-hole components

* Keyboard Maintainer: [CrimsonKeyboards](https://github.com/DeeDesired)
* Hardware Supported: Resume1800, atmega32a

Make example for this keyboard (after setting up your build environment):

    make crimsonkeyboards/resume1800:default

Flashing example for this keyboard:

    make crimsonkeyboards/resume1800:default:flash

How to enter the bootloader:
* 1) Press and hold BOOT
* 2) Press and release RESET
* 3) Release BOOT

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
