# chromatonemini

![chromatonemini](https://i.imgur.com/SuXzf9Dh.jpg)

chromatonemini keyboard is a simple-design Chromatone mini MIDI keyboard that covers 3 octaves (37 notes).

* Keyboard Maintainer: [3araht](https://github.com/3araht)
* Hardware Supported: chromatone keyboard, a DIY MIDI keyboard.
* Hardware Availability: [BOOTH](https://3araht.booth.pm/). Click [here](https://www.tenso.com/en/static/lp_shop_booth) for BOOTH overseas shipping!

Make example for this keyboard (after setting up your build environment):

    make chromatonemini:default

Flashing example for this keyboard:

    make chromatonemini:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
