# ANAVI Macro Pad 12

ANAVI Macro Pad 12 is a compact mechanical keyboard with hot-swappable Cherry MX compatible mechanical switches, translucent keycaps, USB-C, RP2040 microcontroller, backlighting and under lighting.

* Keyboard Maintainer: [Leon Anavi](https://github.com/leon-anavi)
* Hardware Supported: ANAVI Macro Pad 12
* Hardware Availability: [Crowd Supply](https://www.crowdsupply.com/anavi-technology/anavi-macro-pad-12-and-arrows), [GitHub repository](https://github.com/AnaviTechnology/anavi-macro-pad-12)

Make example for this keyboard (after setting up your build environment):

    qmk compile -kb anavi/macropad12 -km default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

Enter the bootloader in 3 ways:

* **Bootmagic reset**: Hold down the top left key on the left half, or top right key on the right half, and then plug in the USB cable on that keyboard half.
* **Physical reset button**: Double tap the reset button on the XIAO RP2040.
* **Keycode in layout**: Press the key mapped to `QK_BOOT` if it is available.
